천안시영상미디어센터

퍼블릭억세스 장비 구입  물품 규격 시방서

2008. 5

www.cdcia.net

제1장 일반사항

1. 사업 개요

가. 사업명 : 천안시영상미디어센터 인테리어공사

나. 건물위치 : 천안시 원성동 261-18번지

다. 규 모

1) 대지면적 : 3,602.00m2

2) 층    수 : 1동, 지상2층 ~ 5층

3) 건축면적 : 721.35 m2

4) 연 면 적 : 1,790,98m2

5) 설계면적 : 872.87m2

2. 제안요청사항

구분			구성장비 계획	비고
2층	만 남	운영 사무실	- 보안장비 및 기타
		다목적강의실	- 프로젝터, 전동스크린, 블루 스크린 및 기타
		아카이브실	- LCD Displayer - DVD & VHS Recorder - 헤드폰 및 기타
3층	체 험	장비 대여실	- HDV급 Camcorder - 조명장비, 사운드 장비 - 찾아가는 미디어 교실 장비 및 기타
		오디오스튜디오	- 디지털 오디오 콘솔 - DA NLE Workstation - 마이크, 스피커 및 기타
		고급편집실	- Mac 기반 NLE System - Certified Digital NLE System - HDV용 VCR 및 SW
		일반편집교육실	- Certified Digital NLE System - HDV용 VCR 및 SW Projecter
4층	소 통	상영관	- 4K Digital Projector - HDV/DV Players - Sound in/out Tools - Auxiliary Itmes

3. 계약일반사항

1) 시방의 목적

본 시방은 미디어센터를 구축함에 있어서, 시민들이 쉽게 접근할 수 있고 운용이     편리한 시스템을 구축하고, 센터의 영역별 사업을 원활하게 수행하기 위해 이를 수    행하는 계약회사 간에 필요한 일반적인 사항을 규정하는데 목적을 둠.

2) 사업기간 및 중점사항

- 사업기간 : 계약일 ~ 2008년 7월 25일까지

단, 특수한 사정이 있을 시는 "갑"과 "을"이 협의하여 조정함.

- 구축장소는 충남디지털문화산업진흥원측이 지정하는 장소로 한다.

3) 적용 법령 및 기준

교육 영상장비의 납품․설치다음의 법령과 기준 등을 참조하여 제작 및 설치되어야 함.

- 장비 품목명세 및 시방서

- 장비 구입 및 설치 시방서

- 기술기준

- 전기용품 안전관리법

- 기타 관계 법령 및 규정

4) 기자재의 납품 및 설치

- 계약자는 본 사업범위 내 계약품목에 대해 본 시스템이 원활히 작동 가능하         도록 설치작업까지 수행하여야 하며 필요 할 경우 주변장비들과의 호환 및  연      동에 필요한 설치작업도 포함하여야 한다.(기존 보유 장비 포함)

- 계약자는 본 사업과 관련한 계약서상의 물품(장비,소프트웨어 등)의 경우

수입품의 경우는 관계 법령에 의거 정식 통관된 물품으로 납품하여야 함.

-  계약자는 본 사업과 관련한 계약서상의 물품(소프트웨어)의 경우 제조자로           부터 라이선스를 인정받은 정품으로 납품하여야 한다.

- 제조품 또는 국내 생산품의 경우 안전 및 국내 관계법에 의거하여 제작된               제품을 납품하여야 함.

- 모든 설치 방법 및 관련 잡자재 등은 소방법 등 관계 법령에 저촉되지 않           도록 시공하여야 함.

-  교육용 영상장비 납품 및 설치는 일반대중 소장 정보장치와 연계하여 실무          운용교육과 활용이 용이하여야 하며, 정보인프라 네트워크 참여가 가능하            도록 설치되어야 함. 또한 다양한 프로그램 Package를 다룰 수 있도록 구축 하여야 함.

4. 검수사항 및  사후관리

1) 출고 전 검사

- 주요 기자재는 공장출고 전에 제조회사에서 성능시험을 거처 "갑"에 납품 하여야 함.

2) 인수 후 검사

- "을"은 납품된 기자재의 설치 시, 기자재의 정상작동 여부를 "갑"의 입회하에 실시해야 함.

- 본 검사에서 문제가 발생될 경우에는 "을"의 책임 하에 원상 복구하거나 교환하여야 함.

다만, "갑"의 과실로 인한 것은 예외로 함.

3) 하자보증

- 퍼블릭억세스에 관한 하자보증 기간은 납품일로부터 계산하여 1년으로 하며         이 기간 동안에 발생한 장비의 자연 고장은 무상으로 수리하여야 함.

단, "갑"과 "을" 쌍방이 합의하는 소모성 부품 및 “갑”의 과실로 발생한 고 장의 경우는 예외로 함.

4) 기술교육 실시

- 본 공사 계약자는 설치되는 영상장비의 원활한 운영을 위하여 운용자들에           대하여 다음과 같은 기술교육을 실시해야 함.

- 대 상 : 시스템 운용 및 Software 운용 교육

- 기 간 : "갑"이 지정

- 인 원 : 해당 인원 10명 이내

5) 장비 기술설명서

- 납품되는 장비의 원활한 운영과 보수 유지를 위하여 특별히 명시하지 않더          라도 장비설명서를 반드시 첨부하여 납품하여야 함.

5. 각 실별 장비구축의 방향

1) 다양한 교육 당사자들을 고려한 최적의 환경이여야 한다.

2) 장애인 편의시설을 설치함에 있어서, 물리적 정서적 접근권을 고려하여야

한다.

3) 독립건물로써의 운영 및 관리에 있어 다양한 측면을 고려하여야 한다.

4) 각 실별 동선 및 사용자들의 활동을 고려하여야 한다.

5) 센터운영 및 디지털영상기술의 발전에 따른 업그레이드를 고려하여야 한다.

6. 제조사 공급증명원 및 A/S 기술 지원확약서 제출 장비 목록

지정 장비
일반편집 교육실	디지털 편집장비 시스템(하드웨어/소프트웨어), HDV VCR, Projector
고급 편집실	디지털 편집장비 시스템(하드웨어/소프트웨어), HDV VCR, HD 모니터
오디오 스튜디오	디지털콘솔, DAW
장비대여실	디지털캠코더 1,2,3, 로케이션 녹음시스템, XLR , 아답타, DLP 프로젝터, HDV VCR
사무실	DID S/W
상영관	4K Digital Projector, HDV VCR, 5.1Ch Speaker, AMP
다목적 강의실	프로젝터

제2장  미디어센터 층별 공간 활용 목적 및 방향

공 간	목 적	방 향
1층	만남	영상미디어센터를 처음 방문한 지역주민 및 공동체가 영상미디어가 가진 특성과 의미를 이해하는 공간 개념
2층	체험	영상미디어와 만남의 경험을 통하여 영상미디어를 기획하고 제작하여 자신을 표현하는 공간 개념
3층	소통	영상미디어를 통해 타인과 지역 그리고 세상과의 소통의 가치를 실현하는 공간 개념

1. 일반편집 교육실

가. 기능

1) 강사 1인, 학생 20인이 영상미디어 이론 교육을 위하여 사용할 수 있는

워크스테이션을 구비하여 영상미디어 강의를 수행 할 수 있도록 구성한다.

2) 구축되는 소프트웨어와 하드웨어는 인증 받은 제품으로 안정성과 신뢰성을            확보하여야 한다.

3) 모든 영상신호는 Beam Projector를 통해 볼 수 있도록 구성한다.

4) VCR장치는 I link 인터페이스를 통해 2 : 1로 공유되며, 녹화, 재생되도록

구성한다.

나. 주요장비

1)  Certified Digital NLE System

2)  HDV용 VCR

3)  음향시스템

4)  LCD-Projecter

5)  기타

2. 고급 편집실

가. 기능

1)  일반편집실의 기본 편집교육과 연계된 전문편집을 위한 공간으로 손색이

없어야 한다.

2)  각종 2D 그래픽 툴 및 동영상 편집 S/W를 구동하는데 문제가 없어야 한다.

3)  VCR장치는 상호 공유되며, 녹화, 재생되도록 구성한다.

4)  비선형편집시스템은장기적으로 HD급 편집도 가능한 시스템으로 구축

하여야 한다.

나. 주요장비

1)  Mac 기반 NLE System 1종

2)  Certified Digital NLE System 2종

3)  HDV용 VCR

4)  편집용 SW 2종 (Mac 컴퓨터 기반의 S/W 포함 )

5)  기타

3. 오디오 스튜디오

가. 기능

1)  콘텐츠의 오디오 편집을 위하여 디지털 믹싱 시스템을 구축한다.

2)  원활한 오디오편집을 위하여 최신의 오디오편집 소프트웨어를 구성한다.

3)   다양한 포맷의 오디오 입․출력 장비를 구성하여 여러 환경에 유연성 있는

시스템을 구비한다.

나. 주요장비

1)  디지털 믹싱 콘솔

2)  오디오 Workstation

3)  오디오 패치 등

4)  오디오 녹음 장치

5)  기타

4. 장비대여실

가. 기능

1)  지역주민 및 공동체가 자유롭게 다양한 형태의 창작 활동을 지원 하도록 다수의

동영상 촬영 장비 및 음향장비, 조명 장비를 구비한다.

2)  장비대여 및 찾아가는 미디어 교실의 운영을 고려하여 각 장비와 악세사리 등을

SET 개념으로 구축한다.

나. 주요장비

1)  HDV급 Camcorder 외

2)  각종 Camcorder 악세사리 일체

3)  Lighting System

4)  각종 사운드 장비 일체

5)  디지털 카메라 일체

6)  찾아가는 미디어 교실 운영장비

5. 운영 사무실

가. 기능

1)  영상미디어센터 운용에 필요한 보안 시스템을 구축한다.

2)  영상미디어센터의 효율적인 운영 및 관리를 위한 고려를 하여야 한다.

3)  사용자를 위한 무선 인터넷 시스템 환경을 제공한다.

4)  DID 시스템을 설치하여 미디어센터에 대한 안내와 전시, 상영 안내 및

홍보 영상을 상영한다.

나. 주요장비

1)  DID 시스템

2)  CCTV 보안 장비 일체

6. 상영관

가. 기능

1)  지역 주민 및 시민들이 자유롭게 다양한 내용의 영상자료를 감상할 수

있도록 한다.

2)  교육 결과물에 대한 시사실 기능 및 배급 효과를 도모하도록 한다.

3)  지역 주민과 공동체가 영상문화복지를 공유하는 열린 공간으로 활용한다.

4)  디지털 영사기는 고해상도 D-Cinema용 DLP 칩을 사용한 4K Digital

Projector로 상영관 수준의 영상을 제공한다.

5)  상업용 극장 수준의 오디오 시스템 수준으로 구축하여야 한다.

나. 주요장비

1)   4K Digital Projector

2)   HDV/HDD/Bluelay  등의 다매체 Players

3)   5.1CH Sound Systems

4)  Auxiliary Items

7. 아카이브 구축

가. 기능

1)  지역 주민 및 시민들이 자유롭게 다양한 내용의 영상자료를 감상할 수 있도

록 한다.

2)  미디어 자료실은 동시에 6인(2인*2,1인*2)이 감상할 수 있도록 구축 하여야

하며, 그에 맞는 영상 및 음향 장비들을 구축하여야 한다.

나. 주요장비

1)  LCD  Displayer

2)  DVD & VHS Recorder

3)  헤드폰

4)  기타

8. 다목적 강의실

가. 기능

1)  영상미디어관련 이론 강의를 할 수 있는 공간으로 구축한다.

2)  지역 주민 및 공동체의 네트워크 구축을 위한 회의실로 활용될 수 있어야

한다.

3)  간이 스튜디오로 활용 할 수 있는 공간과 장비 구성을 고려하여야 한다.

나. 주요장비

1)   Projector

2)   이동용 책, 걸상 배치

3)   5.1채널 음향장비 시스템

4)  전동 블루스크린

9. 인터넷 공유망 구축

가. 기능

1) 미디어센터 전 구역을 무선 인터넷 영역으로 구성한다.

2)  각 실 별 엑세스포인트의 암호화 설정 기능을 보유하여 보안 등급에

따른 접속 통제가 가능하도록 한다.

3) 사무인력의 공간은 안정성을 위하여 유선화 시공한다.

나. 주요장비

1) 무선 Acess Point

2) Hub 등

제 3 장  장비 세부 목록

(※는 제조사 공급증명원 및 A/S 기술 지원확약서 제출 )

1. 일반편집교육실 (58.94㎡)

번호	품목	수량	단위	비고
일-1	OpenHD Certified Workstation	21	ea	※
일-2	LCD Monitor for Workstation	21	ea
일-3	OpenHD NLE Education S/W	21	set
	- Premiere CS2+CS3	21	ea
	- After Effect CS2+CS3	21	ea
	- Photoshop CS2+CS3	21	ea
	- Sound Booth CS2+CS3	21	ea
	- Illustrator CS2+CS3	21	ea
	- Flash CS2+CS3	21	ea
	- Encore CS2+CS3	21	ea
	- On Location CS3	21	ea
일-4	V3 (Enterprise)	21	ea
일-5	W/L Lancard	21	ea
일-6	HDVCAM VCR	11	ea	※
일-7	Projector	1	ea
일-8	Elec. Screen	1	ea
일-9	Audio System	1	set
일-10	Speaker	1	pair
일-11	Headphone	21	ea
일-12	AVRack	1	ea
일-13	Education Desk for 2 man	10	ea
일-14	Education Desk for 1 man	1	ea
일-15	Chair	21	ea
일-16	Install & Materials	1	lot

2. 고급편집실 (31.07㎡)

번호	품목	수량	단위	비고
고-1	NLE Workstation	1	ea	※
고-2	Cinema HD Display	1	ea
고-3	NLE S/W 1	1	ea
고-4	Open HD Certified Workstation	2	ea
고-5	LCD Monitor for Workstation	2	ea
고-6	NLE S/W 2	2	ea
고-7	HD Editing Board	1	ea
고-8	V3 (Enterprise)	3	ea
고-9	W/L Lancard	3	ea
고-10	HD Monitor	1	ea	※
고-11	HDVCAM VCR 1	3	ea
고-12	Headphone	6	ea
고-13	NLE Desk	3	ea
고-14	Chair	6	ea
고-15	Install & Materials	1	lot

3. 오디오 스튜디오 (36.35㎡)

번호	품목	수량	단위	비고
오-1	Digital Audio Mixing Console	1	set	※
	- Meter Bridge	1	ea
	- Side Panel	1	ea
오-2	DA NLE Workstation	1	set
오-3	Multi Rec. S/W	1	ea
오-4	LCD Monitor	2	ea
오-5	Viewing Monitor	1	ea
오-6	AV Option	1	ea
오-7	CDP	1	ea
오-8	Midi Interface	1	ea
오-9	Reverb	1	ea
오-10	Headphone Amp.	1	ea
오-11	Condensor Mic.1	1	ea
오-12	Dynamic Mic.1	2	ea
오-13	Headphone	4	ea
오-14	Mic Stand	3	ea
오-15	Synthesizer	1	ea
오-16	Monitoring Speaker	2	ea
오-17	Music Accompaniment machine	1	ea
오-18	Audio Rack Desk w/ Chair	1	set
오-19	Sub Desk Rack	1	set
오-20	Wall Panel	1	ea
오-21	Audio Patch Bay	1	ea
	- Patch Cord	10	ea
오-22	Tally Controller	1	ea
오-23	On-Air Lamp	3	ea
오-24	Installation and Cabling Works	1	lot

4. 장비대여실 (26.01㎡)

번호	품목	수량	단위	비고
장-1	Digital Camcorder 1	2	set	※
	- Large Battery	2	ea
	- Quick Charger	1	ea
	- UV Filter	2	ea
	- Case	2	ea
장-2	Digital Camcorder 2	8	set
	- Large Battery	8	ea
	- Wide Converter Lens	2	ea
	- UV Filter	8	ea
	- Quick Charger	4	ea
	- Hard Case	8	ea
장-3	Digital Camcorder 3	11	set
	- Spare Battery	11	ea
	- Case	11	ea
장-4	Tripod 1	2	set
	- Fluid Head	2	ea
	- Tripod	2	ea
	- Half ball	2	ea
	- Carrying Bag	2	ea
	- Portable Dolly	2	ea
장-5	Tripod 2	8	ea
장-6	Digital Still Camera(DSLR)	2	ea
	-Lens	2	ea
	- Battery	2	ea
	- Memory	2	ea
	- Case	2	ea
장-7	Wide Single Lens	1	ea
장-8	Zoom Lens	1	ea
장-9	Digital Camera	21	set
	- Memory	21	ea
	- Rechageble Set	21	ea
	- Case	21	ea
장-10	Two Way Light	6	ea
	- Lamp	6	ea
	- Lamp	6	ea
	- Carrying Case	2	ea
장-11	Video Light	2	ea
장-12	Reflector	5	ea
장-13	Gelatine	1	roll
장-14	Locational Sound System	1	sys	※
	-Headphone	1	ea
	-Boompole	1	set
	- Location Mic	1	set
	-Suspensionpistolgrop,	1	ea
	-Hairycover	1	ea
	-Bascketwindshield	1	ea
	- Carrying aluminum box	1	set
	-10mM/F XLR connectedcable	1	ea
장-15	Audio Recorder	1	set
	- Field Case	1	ea
장-16	Other Equipments for Recording	5	set	※
	- XLR Adaptor	5	ea
	- Boom Pole	5	ea
	- Boom Microphone	5	ea
	- XLR Cable	5	ea
	- Voice Recorder w/Pin Mic.	5	ea
장-17	Film Slate	5	set
장-18	Carrier	2	ea
장-19	Rain cover	2	ea
장-20	Portable DV Deck	2	ea
장-21	WalkyTalky	8	ea
장-22	16Ch W/L Mic.	10	ea
장-23	Steady Cam	1	ea
장-24	Wheelchair Tripod	5	ea
장-25	I Type office Desk	1	ea
	- Chair	1	ea
	찾아가는미디어교실
장-26	NLE NoteBook	6	ea
장-27	DLP Projector	2	set	※
	- Carrying Case	2	ea
장-28	Portable Film Screen	2	ea
장-29	Audio System	2	ea
장-30	Video Deck	2	set	※
	- Carrying Case	2	ea
장-31	V3(Enterprise)	6	ea

5. 운영 사무실 (56.4㎡)

번호	품목	수량	단위	비고
사-1	CCTV Camera	9	ea
사-2	DVR	1	ea
사-3	Monitor	1	ea
사-4	2F,3F,4F W/L internet System	1	sys.
사-5	DID system	1	ea	※

6. 상영관 (180.48㎡)

번호	품목	수량	단위	비고
상-1	4K Digital Projector	1	ea	※
	- Zoom Lens	1	ea
상-2	Projector Rack	1	ea
상-3	W/L Mic(Pin Type)	1	ea
상-4	Wired mic.	4	ea
상-5	Mic Stand	4	ea
상-6	Bluelay Player	1	ea
	-Converting Gender	1	ea
상-7	HDV Player	1	ea	※
상-8	HDD Player	1	set
상-9	LCD Viewing Monitor	1	ea
상-10	Audio Monitor	1	pair
상-11	Headphone	1	ea
상-12	Audio Mixer	1	ea
상-13	Surround 7.1Ch Amp	1	set
상-14	3-way main stage speaker	3	ea	※
상-15	Subwoofer speaker	1	ea
상-16	Surround speaker	6	ea
상-17	- Surround bracket	6	ea
상-18	Power Amp.	5	ea
상-19	Micro Hall Screen	1	ea
상-20	Screen Protector	1	ea
상-21	AL Rack	1	ea
상-22	I Type office Desk	1	ea
	- Chair	1	ea
상-23	Installation& Materials	1	lot
	- including Mike Wall box	2	ea

7. 아카이브실 (23.04㎡)

번호	품목	수량	단위	비고
아-1	LCD Display	4	ea
아-2	DVD/VHS Player	4	ea
아-3	Headphone	6	ea
아-4	Headphone Distributor	2	ea
아-5	Library Desk	4	ea
아-6	Chair 1	2	ea
아-7	Chair 2	2	ea

8. 다목적 강의실/회의실 (67.68㎡)

번호	품목	수량	단위	비고
다-1	Projector	1	ea	※
다-2	Elec. Screen	1	ea
다-3	DVD/VHS Player	1	ea
다-4	5.1 ch Speaker	1	set
다-5	W/L Mic w/ Pin&Handheld	1	set
다-6	AV Processor	1	set
다-7	Mixer	1	ea
다-8	A/V Rack	1	ea
다-9	Education Foldable Desk	10	ea
다-10	Education Foldable Chair	30	ea
다-11	Blue Screen	1	ea
다-12	Auto Pole	1	pair

일반 편집 교육실

규    격    서

ITEM NO.	품명	수량
일-1	Open HD Certified Workstation	21ea

규격	세부사양	비고
세부규격	- CPU : Intel Core 2 Duo Processor E8400/3.00GHz 6MB/1333MHz FSB - Chipset : Intel X38 Express chipset - Graphic : NVIDIA Quadro FX570 256MB PCIe Graphics - Memory : 2GB(2*1GB) DDR2-800 ECC RAM (4*Memory DIMM, 최대 8GB 지원) - HDD1 :160GB SATA 3Gb/s NCQ 7200rpm HDD (최대 4*SATA HDD, 최대 2TB 지원,2 will require optional expander kits) - HDD2 : 250GB SATA 3Gb/s NCQ 7200rpm HDD - Bay : 3*External 5.25 in. Bay, 1*External 3.5 in. Bay, 2*Internal 3.5 in. Bay, Floppy Disk Drive - ODD : 16X DVD+-RW SuperMulti SATA Drive - Integrated Serial-ATA controller 3Gb/s (NCQ with 5 SATA connectors), with RAID 0, 1, 5 and 10 capability - Integrated Broadcom 5755 NetXtreme Gigabit PCIe LAN - Integrated high definition audio with jack retasking capability - USB Optical Scroll Mouse & USB Standard KeyBoard, IEEE 1394a - FireWire 3-Port PCI Card - Roxio Easy Media Creator version 9 - Intervideo WinDVD Software - Protect Tools Security Manager - Roxio Easy Media Creator Ver.9 - Intervideo WinDVD Software - Performance Tuning Framework - Backup and Recovery Manager - 2*PCI Express (PCIe) x16 graphics,1*PCIe x8 (x4 electrical) slot, 1*PCIe x1 slot, 3*PCI slots - Dimensions(H*W*D) : 44.9cm(17.7 in)*17.0cm(6.7 in)*45.7cm(18.0 in) - Power Supply : 475 watts - HP xw4600 80+ Energy Efficient Chassis - OS : Microsoft Vista32B Downgrade to XP32B OS	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
일-2	LCD Monitor for Workstation	21ea

규격	세부사양	비고
세부규격	- Display size (diagonal) : 51cm (20") - Display type : Active matrix TFT - Resolution : 1680x1050 @ 60 Hz - Response rate (typical) : 5ms - In-put : Analog/Digital - Brightness (typical) : 300 nits - Contrast ratio (typical) : 800:1 - Viewing angle : 160/160 - Frequency range (horizontal) : 24 - 93 kHz - Frequency range (vertical) : 50 - 76 Hz - Pixel Pitch(mm) : 0.258mm B - Synch input : TTL separate synch or Composite Sync - Ports : Rear - 2x USB 2.0 - Dimensions (w x d x h) : 18.56 x 8.78 x 18.85 in (47.14 x 22.3 x 47.89 cm) - Weight : 16.7 lb (7.68 kg)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
일-3	OpenHD NLE Education S/W	21set

규격	세부사양	비고
세부규격	개요 : - HD/HDV 편집의 공식 인증 시스템 - 안정적인 HDV 넌리니어 편집/교육 시스템 - 다양한 영상 편집과 어떠한 포맷에도 대응 가능한 범용 교육이 가능한 유연성있는 시스템 구성 : Adobe After Effects® CS2 + CS3 Professional / Adobe Premiere® Pro CS2 + CS3 Adobe Photoshop® CS2 + CS3 Extended / Adobe Flash® CS3 Professional Adobe Illustrator® CS2 + CS3 / Adobe Soundbooth™ CS2 + CS3 Adobe Encore® CS2 + CS3 / Adobe OnLocation™ CS3 (Windows® only) Adobe Ultra® CS3 (Windows® only)Adobe® Creative Suite® 3 Production Premium software combines 신속한 워크플로우 Windows/MAC에서 사용 가능 Adobe Bridge를 사용한 파일 검색 및 구성 32비트 레이어 및 페인팅 등 HDR(High Dynamic Range) 색상 지원 DV, SD, HDV 및 HD와의 호환성, 다양한 업계 표준 및 포맷 지원 FLV 파일 내보내기 우수한 32비트 오디오 파이프라인 Adobe After Effects를 사용한 모션 그래픽 및 시각적 효과 퍼핏 툴을 사용한 직관적인 애니메이션 제작 애니메이션을 바로 제작할 수 있도록 해주는 Brainstorm 작업 시간을 절약할 수 있는 애니메이션 및 동작 사전 설정 매끄럽고 선명하게 그리고 최대 자연스럽게 장면을 느리게 또는 빠르게 조정할 수 있는 Timewarp 효과 Adobe Premiere Pro를 사용한 실시간 비디오 편집 지능적인 파일 검색 기능이 있는 멀티 프로젝트 패널 DV에서 비압축 HD에 이르기까지 전문 포맷 지원 멀티캠 편집, AAF(Windows 전용) 및 EDL 가져오기/내보내기 GPU 가속화 렌더링	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
일-3	OpenHD NLE Education S/W	21set

규격	세부사양	비고
세부규격	Adobe Photoshop을 사용한 이미지 편집 동영상 페인트, 사용한 이미지 편집 3D 이미지 지원 및 텍스처 편집 Adobe Flash를 사용한 인터랙티브 컨텐츠 제작 QuickTime 워크플로우, ActionScript™ 3.0 언어로 변환되는 애니메이션 Illustrator 스타일의 펜 툴을 비롯한 새로운 드로잉 툴 Adobe Illustrator CS3를 사용한 드로잉 및 일러스트레이션 필름 및 비디오 문서 사전 설정 라이브 색상, 포괄적인 드로잉 툴 Adobe Soundbooth를 사용한 오디오 제작 사용자 정의 가능한 Soundbooth 스코어가 포함된 AutoComposer 신속한 마스터링 및 음성 기능 향상 Adobe Encore를 사용한 전문 DVD 및 블루레이 디스크 제작 Flash CS3를 열지 않고도 한 번에 DVD 및 블루레이 디스크 제작 Adobe OnLocation CS3 (Windows 전용) 디스크에 직접 기록, 전문적인 설정 모니터링 Adobe Ultra를 사용한 빠르고 효과적인 키잉 (keying) 작업 (Windows 전용) 품질이 좋지 않은 장면 작업 시에도 고품질의 신속한 키잉 작업 실제 사물과 같은 합성물에 키잉 처리된 장면을 삽입할 수 있는 가상 세트 ** 교육의 유연성을 위하여 지정 품목의 경우 CS2 와 CS3 업그레이드를 패키지 형태로 제공하여야 함.	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
일-4	V3 (Enterprise)	21ea

규격	세부사양	비고
세부규격	- 바이러스, 웜, 해킹, 스파이웨어 등 각종 악성코드 방역 - 개인정보 보호에 탁월 - 피싱 차단 - 네트워크 감염자 추적 / 차단 - 시스템 취약점 관리를 통한 사전 방역 - 시스템 최적화 기능을 통한 깨끗한 컴퓨팅 환경 구현 - 실시간 보안 기능으로 빈틈없는 방역 - 누구라도 손쉽게 사용할 있는 편리한 사용법 - 시스템의 보안 상태를 한눈에 볼 수 있는 편리한 UI - 운영체제 : Windows Vista, Windows 2000/XP, Windows 98 - CPU : Pentium III 700 Mhz Pentium II 266 Mhz - Memory : 256MB, 128MB - HDD : 300MB, 100MB - Screen Size : 1024 * 768, 800 * 600 - CD-ROM : 24배속 4배속 - IE Version : IE 5.0 이상

규    격    서

ITEM NO.	품명	수량
일-5	W/L Lancard	21ea

규격	세부사양	비고
세부규격	- 인터페이스타입 : PCI - 최대속도 : 54Mbps - 무선규격 : IEEE 802.11b, IEEE 802.11g - 주파수대역 : 2.4GHz - 지원OS : Windows 98, Windows 2000, Windows XP, Windows Vista - 보안 : WEP, WPA, CCX 2.0

규    격    서

ITEM NO.	품명	수량
일-6	HDVCAM VCR	11ea

규격	세부사양	비고
세부규격	Recording/playback performance Recording format: 1080/60i, 1080/50i, 480/60i (NTSC), 576/50i (PAL) Playout/down conversion format: 1080/60i, 1080/50i, 480/60i (NTSC), 576/50i (PAL), 480/60P, 576/50P, 720/60P, 720/50P Tape speed: HDV/DV SP Max. 18.812 mm/s DVCAM Max. 28.218 mm/s Playback/recording time: HDV/DV SP Max. 276 min with PHDV-276DM cassette, Max. 63 min with PHDVM-63DM cassette, DVCAM Max. 184 min with PHDV-276DM cassette, Max. 41 min with PHDVM-63DM cassette Fast forward/rewind time: Approx. 2 min with PHDV-276DM cassette Input/output connectors/devices Video input/output: BNC x 2 Video signal: 1 Vp-p, 75 Ω unbalanced, sync negative S-video input/output: Mini-DIN 4-pin x 2 Y: 1 Vp-p, 75 Ω unbalanced, sync negative C: 0.286 Vp-p (NTSC), 0.3 Vp-p (PAL), 75 Ω unbalanced, Component video output: BNC x 3, Y: 1 Vp-p (0.3 V, sync negative) Pr/Pb (Cr/Cb): 700 mVp-p (100% color bar), input impedance 75 Ω i.LINK: 4-pin HDMI output: 19-pin (type A), video: 1080/60i, 1080/50i, 480/60i (NTSC), 576/50i (PAL), 720/60P, 720/50P, 480/60P, 576/50P, audio: PCM 48 kHz/16-bit Phones: Stereo minijack (φ3.5 mm), 8 Ω loading LANC: Stereo mini-minijack (φ2.5 mm) Control S: Stereo minijack (φ3.5 mm) Audio input: RCA pin x 2 Input level: -10/-2/+4 dBu, input impedance: min. 47 kΩ unbalanced,max. input level: -10: +18 dBu (approx. 6 Vrms),-2: +24 dBu (approx. 12.5 Vrms), +4: +30 dBu (approx. 25 Vrms) Audio output: RCA pin x 2 Output level: -10 dBu (full bit -20 dB), impedance 47 kΩ, unbalanced in 60i mode, -10 dBu (full bit -18 dB), impedance 47 kΩ, unbalanced in 50i mode Impedance: max. 1 kΩ unbalanced LCD monitor: 2.7-inch type, approx. 211,200 dots (960 x 220), Clear Photo LCD Plus General Mass: Approx. 4.3 kg (9 lb 8 oz) Power requirements: AC 120 V, 60 Hz Power consumption: 12 W (playback mode with LCD monitor on) Operating temperature: 5 to 40°C (41 to 104°K) Storage temperature: -20 to +60°C (-4 to 140°K) Supplied accessories: Remote commander (1), power cord (1), size AA batteries (2), cleaning cassette (1), operating instructions (1)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
일-7	Projector	1ea

규격	세부사양	비고
세부규격	Brightness - ANSI Lumens : 4,000 Contrast Ratio - Full ON/OFF : 500:1 Illumination Uniformity : 85% Imaging System : 0.8" Polysilicon TFT active matrix Panel x 3 Imaging System : Auto: H Sync. 15-100 kHz ~ V Sync. 50-100 Hz Screen Pixels : 1024 x 768 in stripe configuration Lamp : 300W lamp Estimated Lamp Life Hours : 2000 Computer Native Resolution : 1024 x 768 Computer Compatiblity: UXGA (Compression) / WXGA(Compression) / SXGA (Compression) / XGA / SVGA / VGA Computer Formats Supported : 1600x1200 through 640x480 Computer Dot Clock : 140 MHz Computer Image Sizing : Normal or Smart compressed or expanded Amplifier : Monaural 1W rms (T.H.D 10%) Speakers (Built-in) : 2.8cm 1pce Dimensions : 334(W) x 78(H) x 232(D) mm Net weight : 3.3 kg Packaged dimensions : 420(W) x 214(H) x 365(D) mm Packaged weight : 5.4 kg Operating Temperature - Max. : 95F (35C) Operating Temperature - Min. : 41F (5C) Generated Heat : 1314 BTU (331 KC)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
일-8	Elec. Screen	1ea

규격	세부사양	비고
세부규격	- 스크린 재질 : 매트 화이트 (120“) - 반사 계수 : 정면: 0.8± 10% / 측면 : 0.8± 10% - 계폐 방식 : 전동식 - 크기 : 240 X 180Cm (가로X세로)

규    격    서

ITEM NO.	품명	수량
일-9	Audio System	1set

규격	세부사양	비고
세부규격	Rated output *THD figures are power amp stage values Front : 75 W + 75 W (8 ohms, 20Hz - 20kHz) Centre : 75 W (8 ohms, 20Hz - 20kHz) Surround : 75 W + 75 W (8 ohms, 20Hz - 20kHz) Surround back : 75 W + 75 W (8 ohms, 20Hz - 20kHz) IN-put : HDMI, Component, S-Video, Composite, Analog audio, Digital OPT, Digital COAX, iPod ready Out-put : HDMI, Component, S-Video, Composite, Analog audio, Pre out 0.1ch Input sensitivity/impedance : Audio inputs - 200 mV/47 kohms Output level/Load impedance : Rec. Audio outputs - 200 mV/47 kohms Power supply : AC 230 V, 50 Hz Dimensions (WxHxD) : 434 x 171 x 383 mm Weight : 10.9 kg

규    격    서

ITEM NO.	품명	수량
일-10	Speaker	1pair

규격	세부사양	비고
세부규격	정격출력 : 100 W 로우 응답 주파수 : 55 Hz ~ 22 KHz 감도 : 88 dB 임피던스 : 6 Ω 크로스오버 : 3 KHz 크기(HWD) : 300 x 170 x 200 mm 무게 : 5 Kg

규    격    서

ITEM NO.	품명	수량
일-11	Headphone	21ea

규격	세부사양	비고
세부규격	Closed, dynamic, supra-aural headphones High efficiency drivers Wind-up belt clip for excess cable 10 foot Y style cable Replaceable leatherette ear pads Jack plug: 3.5/6.3 mm stereo Nominal impedance: 32 Ohm Weight w/o cable: ca. 130 g Transducer principle: Dynamic, closed Ear coupling: Supraaural Cable length: 3 m Frequency response (headphones): 18-18000 Hz Sound pressure level (SPL): 115 dB(SPL) THD, total harmonic distortion: Less than 0.5 percent

규    격    서

ITEM NO.	품명	수량
일-12	AV Rack	1ea

규격	세부사양	비고
세부규격	홈시어터, DVD, VDP 기기용 이동바퀴 : 블랙, 월넛 제품크기 : 가로 600 x 높이 860 x 깊이 420 상판유리 : 10T 평유리 선반유리 : 8T 평유리 2장 (높낮이조절 가능) 재질, 마감 : Chamber / 평유리 / 크롬장식 / DIY

규    격    서

ITEM NO.	품명	수량
일-13	Education Desk for 2 man	10ea

규격	세부사양	비고
세부규격	- 일반편집교육실에 구축되는 워크스테이션을 활용할 수 있는 책상 - 피교육자의 공간이 충분히 확보될 수 있어야 함. (장애인교육자의 공간 확보) - PC사용자에게 다양한 모니터 위치(각도)를 제공 - PC본체 및 관련장비를위한 도난방지 구조. - 테이블 자체 전선처리가 용이한 구조. - LCD 모니터 전용으로 설계 된 컴퓨터 책상(LCD 모니터 잠금 장치) - 책상사용인원수 : 2인/세트 - 상판두께 : 28mm - 크기 : 1800(L)*750(H)*720(W) - 몸체 : 재질 PB,LPM 18T Deco Sheet 처리 - 상판 : 재질 PB,LPM 18T Deco Sheet 처리 - 뒷판 : 질 PB,LPM 18T Deco Sheet 처리 - 높이조절기능 : 유 - 전면은 20파이 봉으로 도난 방지 - 키보드 및 마우스 선반 * 색상은 협의 후 지정

규    격    서

ITEM NO.	품명	수량
일-14	Education Desk for 1 man.	1ea

규격	세부사양	비고
세부규격	- 일반편집교육실에 구축되는 워크스테이션을 활용할 수 있는 책상 - 피교육자의 공간이 충분히 확보될 수 있어야 함. - PC사용자에게 다양한 모니터 위치(각도)를 제공 - PC본체를 위한 도난방지 구조. - 테이블 자체 전선처리가 용이한 구조. - LCD 모니터 전용으로 설계 된 컴퓨터 책상(LCD 모니터 잠금 장치) - 책상사용인원수 : 1인/세트 - 상판두께 : 28mm - 크기 : 900(L)*750(H)*720(W) - 몸체 : 재질 PB,LPM 18T Deco Sheet 처리 - 상판 : 재질 PB,LPM 18T Deco Sheet 처리 - 뒷판 : 질 PB,LPM 18T Deco Sheet 처리 - 높이조절기능 : 유 - 전면은 20파이 봉으로 도난 방지 - 키보드 및 마우스 선반 * 색상은 협의 후 지정

규    격    서

ITEM NO.	품명	수량
일-15	Chair	21ea

규격	세부사양	비고
세부규격	안락하고 편안한 구조로 PC사용자에게 편안한 사용이 가능 LCD 컴퓨터 실습용 테이블과 인테리어적으로 조화 크롬 도금 및 스테인레스 재질로 튼튼하고 안전한 구조 장시간 앉아 있어도 편안한 설계. 심플한 디자인의 팔걸이는 발포 우레탄 소재 사용 성형 우레탄 스폰지 위 천 마감 중간 등받이 스틸파이프에 의한 탄력 제공 팔걸이유 크기 : 575×610×890 몸체재질 : POLY PROPYLENE 기타 부품 포함. 색상은 협의후 지정

규    격    서

ITEM NO.	품명	수량
일-16	Install & Materials	1lot

규격	세부사양	비고
세부규격	- Equipment Setting - Cable Connecting - Cable Wiring - S/W Installation - Warranty Service - Hiding Cable - Fixing Equipment - S/W Installment/Testing - H/W Testing - Desk & Chair Setting

고급 편집실

규    격    서

ITEM NO.	품명	수량
고-1	NLE Workstation	1ea

규격	세부사양	비고
세부규격	Processor Two 2.8GHz Quad-Core Intel Xeon (8-core) Memory 2GB (2 x 1GB) HDD 320GB 7200-rpm Serial ATA 3GB/s Graphic ATI Radeon HD 2600 XT 256MB (Two dual-link DVI) ODD One 16x SuperDrive Apple Mighty Mouse Apple Keyboard Two FireWire 800 ports (one on front panel, one on back panel) Two FireWire 400 ports (one on front panel, one on back panel) Five USB 2.0 ports (two on front panel, three on back panel) Two USB 2.0 ports on included keyboard Front-panel headphone minijack and speaker Optical digital audio input and output TOSLINK ports Analog stereo line-level input and output minijacks PCI Express expansion Three open full-length PCI Express expansion slots One PCI Express 2.0 x16 slot Two PCI Express x4 slots All slots provide mechanical support for 16-lane cards 300W combined maximum for all PCI Express slots Software Mac OS X v10.5 Leopard (includes Time Machine, Quick Look, Spaces, Spotlight, Dashboard, Mail, iChat, Safari, Address Book, QuickTime, iCal, DVD Player, Photo Booth, Front Row, Xcode Developer Tools) iLife ’08 (includes iTunes, iPhoto, iMovie, iDVD, iWeb, and GarageBand) Size and weight Height: 20.1 inches (51.1 cm) Width: 8.1 inches (20.6 cm) Depth: 18.7 inches (47.5 cm) Weight (standard configuration): 42.4 pounds (19.2 kg)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-2	Cinema HD Display	1ea

규격	세부사양	비고
세부규격	- Size: 23" diagonal viewable image size - Screen Type: Thin film transistor (TFT) active-matrix liquid crystal display (AMLCD) - Resolutions: 1920 by 1200 pixels (optimum resolution), 1280 by 800 pixels, 1024 by 640 pixels - Display colors (maximum): 16.7 million - Viewing angle (typical): 170? horizontal; 170? vertical - Brightness (typical): 250 cd/m^2 - Contrast ratio (typical): 700:1 - Response time (typical): 16ms - Pixel pitch: 23-inch Cinema HD Display: 0.258 mm - Screen treatment: Antiglare hardcoat - Connectors: Two-port, self-powered USB 2.0 hub, two FireWire 400 ports and Kensington security port - Size and weight : 23-inch Apple Cinema HD Display Height: 17.4 inches (44.3 cm) Width: 20.9 inches (53.3 cm) Depth: 7.3 inches (18.7 cm) Weight: 15.5 pounds (7.03 kg)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-3	NLE S/W 1	1ea

규격	세부사양	비고
세부규격	Real-time editing for DV, SD, HD, and film. - Make videos and movies in any format with Final Cut Pro 5, a major upgrade to Apple's award-winning video editing application. - It features powerful new multicamera editing, native HDV support, precision editing tools, scalable real-time effects processing, advanced real-time color correction and image manipulation filters and audio control surface support. Soundtrack Pro - Precision audio editing. Powerful sound design. - Introducing Soundtrack Pro, - Apple's revolutionary new audio editing and sound design application. - Use action-based editing to creatively design new sounds, instantly repair imperfect location recordings, add perfect sound effects or musical Apple Loops, save hours bringing audio in and out of your video editor thanks to seamless integration with Final Cut Pro and more. Motion 2 - Advanced animation. Instant gratification. - Motion 2 is Apple's award-winning professional motion graphics application offering breakthrough functionality and seamless workflow to artists, editors and independent producers. - Whether you're animating broadcast graphics, corporate presentations, feature film titles, or DVD menus, DVD Studio Pro 4 - Redefining professional DVD authoring. Again. - Whether you produce demo reels, complex commercial titles or anything in between, DVD Studio Pro 4 offers simple, powerful tools for authoring DVDs. - The latest upgrade introduces the next-generation of DVD delivery with HD DVD support for both H.264 and HDV and advanced authoring options like Alpha Transitions and multiple video and audio tracks.	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-4	Open HD Certified Workstation	2ea

규격	세부사양	비고
세부규격	- Dual * Intel Xeon Quad-Core Processor 5430, 2.66GHz, 12MB L2 cache/1333MHz FSB - Chipset : Intel 5400 - NVIDIA Quadro FX1700 512MB PCIe Graphics - 4GB (2*2GB) DDR2-667 ECC (16*Memory DIMM, 최대 128GB 지 원) - 1 * 160GB SATA 3Gb/s NCQ 7200rpm HDD (최대 5*SATA HDD, 최대 5TB 지원) - 2 * 500GB SATA 3Gb/s NCQ 7200rpm HDD - 3*External 5.25 in. Bay, 5*Internal 3.5 in. Bay - Floppy Disk Drive - 16X DVD+-RW SuperMulti SATA Drive - Integrated 6 Channel SATA 3.0Gb/s Controller, RAID 0,1,10,5 capability - Integrated 8 Channel Serial Attached SCSI (SAS) 3.0Gb/s Controller supporting RAID level 0, 1, 10 capability - Dual integrated Broadcom 5755 Netxtreme Gigabit PCIe - High Definition Integrated Realteck ALC262 Audio - 2*PCIe x16 Gen2 Graphics,2*PCIe(x8 mechanically,x4 electrically), 1*PCIe x8 (switchable as x1 or x8), 1*PCI-X 133MHz slot, 1*PCI 32-bit/33MHz Slot - USB Optical Scroll Mouse & USB Standard KeyBoard - Dimensions(H*W*D) : 45.5cm*21.1cm*52.6cm - Power Supply : 800 watts 80 PLUS efficient power supply - HP 2x Standard Heatsink Thermal Kit - Microsoft Vista32B Downgrade to XP32B OS	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-5	LCD Monitor for Workstation	2ea

규격	세부사양	비고
세부규격	Display size (diagonal) : 24 in (61 cm) Display type : Active matrix TFT Viewable area (diagonal) : 24 in (61 cm) Resolution : 1920 x 1200 @ 60 Hz Pixel pitch : 0.27 mm Brightness (typical) : Up to 500 nits Contrast ratio (typical) : Up to 1000:1 Viewing angle : 178 degrees Viewing angle (vertical) : 178 degrees Response rate (typical) : 6 ms Frequency range (horizontal) : VGA input: 30 - 94 kHz; DVI input: 30 - 92 kHz Frequency range (vertical) : VGA input: 48 - 85 Hz; DVI input: 48 - 85 Hz Signal input : Two DVI-I (VGA analog and digital) inputs Ports : Rear - 4 USB 2.0 Bezel color : Carbonite/Silver Tilt Angle : - 5 degrees to + 25 degrees Swivel angle : ± 45 degrees Height adjustable : Range 5.1 in (130 mm) Energy Efficiency : Australian ACA Approval; Canadian Requirements/CSA; CE Marking; CISPR Requirements; Eastern European Approvals; Energy Star Compliant; FCC Approval; ISO 13406-2 Pixel Defect Guidelines; Mexican NOM Approval; Microsoft Windows Certification; PC2001 Compliant; PC99 Certified; S. Korean MIC Approval; Taiwan BSMI Approval; UL Listed; VCCI Approvals; China CCIB/CCEE Approval; Nordic Approvals (Nemko, Fimko, Demko, Semko); ISO 9241-3,7,8 VDT Synch input : Separate sync (HSYNC/VSYNC); composite sync, Sync on Green Dimensions (w x d x h) : 22 x 9.1 x 14.6 in (55.4 x 23.2 x 37.1 cm) (With Stand) Weight : 32.4 lb (14.7 kg)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-6	NLE S/W 2	2ea

규격	세부사양	비고
세부규격	개요 : - HD/HDV 편집의 공식 인증 시스템 - 안정적인 HDV 넌리니어 편집/교육 시스템 - 다양한 영상 편집과 어떠한 포맷에도 대응 가능한 범용 교육이 가능한 유연성있는 시스템 구성 : Adobe After Effects® CS2 + CS3 Professional / Adobe Premiere® Pro CS2 + CS3 Adobe Photoshop® CS2 + CS3 Extended / Adobe Flash® CS3 Professional Adobe Illustrator® CS2 + CS3 / Adobe Soundbooth™ CS2 + CS3 Adobe Encore® CS2 + CS3 / Adobe OnLocation™ CS3 (Windows® only) Adobe Ultra® CS3 (Windows® only)Adobe® Creative Suite® 3 Production Premium software combines ** 교육의 유연성을 위하여 지정 품목의 경우 CS2 와 CS3 업그레이드를 패키지 형태로 제공하여야 함.	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-7	HD Editing Board	1ea

규격	세부사양	비고
세부규격	PCIe 4-lane compatible Look Up Tables ●Real-time primary LUT ●Import/export text-based LUT files File Import/Export : Import (capture) and export (playback) standard file formats: DPX, Cineon, TGA,TIFF, BMP, and AVI, QuickTime, WAV. Video Formats ●SD: 525i 29.97, 625i 25 ●HD: 720p Variable Frame Rate (23.976, 24, 29.97, and 30), 720p 50, 720p 59.94, 720p 60, 1080i 25, 1080i 29.97, 1080i 30, 1080p 23.976, 1080psf 23.976, 1080p 24, 1080psf 24, 1080p 25, 1080psf 25, 1080p 29.97, 1080psf 29.97, 1080p 30, 1080psf 30 Video Input ●Digital: HD-SDI/SDI, SMPTE-259/292/296 ●Analog: SD and HD Input, BNC ●HD: YPbPr, RGB ●SD: YPbPr, RGB (component mode), Composite/YC (composite mode), 12-bit A/D Video Output ●SD and HD Output, BNC ●HD: YPbPr, RGB ●SD: YPbPr, RGB (component mode), Composite/YC (composite mode), 12-bit D/A Audio Input ●Digital: 2-channel 16/24/32-bit AES/EBU, 48kHz sample-rate Synchronous or Non-synchronous (Internal sample-rate conversion) ●16/24/32-bit SMPTE-259 SDI embedded audio, 8-channel, 48kHz synchronous ●Analog: 2-channel balanced input +24dbu Full Scale Digital 16/24/32-bit A/D, 48kHz sample rate +/- 0.2db 20 to 20kHz Frequency Response

규    격    서

ITEM NO.	품명	수량
고-7	Editing Board	1ea

규격	세부사양	비고
세부규격	Audio Output ●Digital: 2-channel 16/24/32-bit AES/EBU, 48kHz sample rate 16/24/32-bit AES/EBU, 48kHz sample rate 16/24/32-bit SMPTE-259 SDI embedded audio, 8-Ch, 48kHz synchronous ●Analog: 2-channel balanced output +24dbu Full Scale Digital 16/24/32-bit D/A, 48kHz sample rate +/- 0.2db 20 to 20kHz Frequency Response Down-Conversion ●Hardware 10-bit output, 16/24/32-bit internal processing ●Anamorphic: full-screen Letterbox: image is reduced with black top and bottom added to image area with the aspect ratio preserved ●Crop: image is cropped horizontally Reference Input ●Analog Color or HD Tri-level ●1 BNC on standard breakout cable (75 ohm terminating) ●KL-Box (optional): 2 BNCs, passive loop Machine Control ●RS-422, Sony 9-pin protocol Connector pro-vided on XENA LH/LHe breakout cable and on optional KL-Box.

규    격    서

ITEM NO.	품명	수량
고-8	V3 (Enterprise)	3ea

규격	세부사양	비고
세부규격	- 바이러스, 웜, 해킹, 스파이웨어 등 각종 악성코드 방역 - 개인정보 보호에 탁월 - 피싱 차단 - 네트워크 감염자 추적 / 차단 - 시스템 취약점 관리를 통한 사전 방역 - 시스템 최적화 기능을 통한 깨끗한 컴퓨팅 환경 구현 - 실시간 보안 기능으로 빈틈없는 방역 - 누구라도 손쉽게 사용할 있는 편리한 사용법 - 시스템의 보안 상태를 한눈에 볼 수 있는 편리한 UI - 운영체제 : Windows Vista, Windows 2000/XP, Windows 98 - CPU : Pentium III 700 Mhz Pentium II 266 Mhz - Memory : 256MB, 128MB - HDD : 300MB, 100MB - Screen Size : 1024 * 768, 800 * 600 - CD-ROM : 24배속 4배속 - IE Version : IE 5.0 이상

규    격    서

ITEM NO.	품명	수량
고-9	W/L Lancard	3ea

규격	세부사양	비고
세부규격	- 인터페이스타입 : PCI - 최대속도 : 54Mbps - 무선규격 : IEEE 802.11b, IEEE 802.11g - 주파수대역 : 2.4GHz - 지원OS : Windows 98, Windows 2000, Windows XP, Windows Vista - 보안 : WEP, WPA, CCX 2.0

규    격    서

ITEM NO.	품명	수량
고-10	HD Monitor	1ea

규격	세부사양	비고
세부규격	Video System : NTSC and PAL, All HDTV Formats and Frame Rates Application : Studio, Broadcast Screen Size : 17.1" Maximum Resolution : 800 Lines Phosphor : Not Applicable Color Temperature Pre-Sets : 5600k, 6500k, 9300k, Full Custom 3000k to 9300k Selectable Input and Output Connectors: ●SDI Video- BNC (x 2 input, 1 output) ●Component Video- 4-BNC (x 1 input, 1 output) ●S-Video- 4-Pin (x 1 input, 1 output) ●Composite Video- BNC (x 2 input, 1 output) ●Audio- RCA (x 2 input) ●RS-232C Control- 15-Pin (x 1) ●GPI- 15-Pin (x 1) - Set-Up Features : Blue Gun, H/V Delay, Monochrome - Power Requirements : 100~230 VAC, 50 or 60 Hz - Power Consumption : 4A	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-11	HDVCAM VCR 1	3ea

규격	세부사양	비고
세부규격	- Recording format HDV: HDV1080/60i, 1080/50i, 1080/24p, 1080/25p, 1080/30p DVCAM/DV SP: DVCAM,DV SP 480/60i (NTSC), 576/50i (PAL) - Playout format HDV: HDV1080/60i, 1080/50i, 1080/24p, 1080/25p, 1080/30p. HDV720/24p, 720/25p, 720/30p DVCAM/DV SP:DVCAM,DV SP 480/60i (NTSC), 576/50i (PAL) - Playout video signal 1080/60i, 1080/50i, 480/60i (NTSC), 576/50i (PAL), 480/60P, 576/50P, 720/60P, 720/50P - Tape speed HDV/DV SP: Max. 18.812 mm/s DVCAM: Max. 28.218 mm/s - Playback/recording time- HDV/DV SP: Max. 276 min with PHDV-276DM cassette Max. 63 min with PHDVM-63DM cassette DVCAM: Max. 184 min with PHDV-276DM cassette Max. 41 min with PHDVM-63DM cassette - Fast forward/rewind time : Approx. 2 min with PHDV-276DM - Video input/output : BNCx1 / BNCx1 - Monitor video out : RCA pin x1 - S-video input/output : Mini-DIN 4-pin x1 / Mini-DIN 4-pin x1 - Component video output : BNC x 3 - i.LINK interface (HDV /DV) : 6-pin (no power) - HD/SD-SDI output : BNC x1 - Audio input : RCA pin x 4ch - Audio output : XLR 3pin x 4ch - Monitor audio out : RCA pin x 1 - AES/EBU output : BNC x2 - TC out : BNC x1	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-11	HDVCAM VCR 1	3ea

규격	세부사양	비고
세부규격	- Phones : Stereo minijack (ø3.5 mm) - LANC : Stereo mini-minijack (ø2.5 mm) - Control S input : Stereo minijack (ø3.5 mm) - LCD monitor : 2.7-inch type (Viewable area measured diagonally), approx. 211,200 dots (960 x 220), Clear Photo™ LCD Plus - Weight : Approx. 9 lb 12 oz (4.4 kg) - Dimensions (WxHxD): Approx. 212 x 88 x 390.3mm - Power requirements : AC 120 V, 60 Hz - Power consumption : 16 W (playback mode with LCD monitor on)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
고-12	Headphone	6ea

규격	세부사양	비고
세부규격	- Connector Type: 1/8 - Weight: 9.9 - Isolation: -15dB - Detachable Cable: No - Impedance @ 1kHz: 64 - Coupler Size: Large - Cord Type: Coiled Left-Side - Cord Length: 10 ft. - Ear Coupler Type: Full-Size - Driver Type: Dynamic - Acoustic Seal: Sealed - Headphone Type: Head Set

규    격    서

ITEM NO.	품명	수량
고-13~14	NLE Desk	3ea

규격	세부사양	비고
세부규격	- HD NLE System을 수용 할 수 있는 사이즈의 편집용 책상. - 2인 동시 편집을 고려 - 색상 등은 공간 구성과 조화 되도록 협의 <참조> 상판 : 내수성 내오염성 및 내열성이 강한 30mm 두께의 M.D.F 위에 1.3mm H.P.M접착. (상판 - 앞경사, 뒤포밍, 양쪽 3mm 엣지처리) 측판 : 23mm두께의 파티칼 BOARD를 사용. 마무리는 3mm P.V.C엣지로 처리. 뒷판 : 18mm두께의 파티칼 BOARD를 사용한다. (마감부분은 3mm P.V.C엣지 처리) 바퀴 : 원형 조절발을 사용. 상판과 측판 연결 부분을 P.V.C 사출물 부속을 사용하여 견고히 결착. 크기 : 2000 x 750 x 720 편집실용 고급의자 : 6ea 포함.

규    격    서

ITEM NO.	품명	수량
고-15	Instatll & Materials	1lot

규격	세부사양	비고
세부규격	Equipment Setting Cable Connecting Cable Wiring Warraty Service Hiding Cable Fixing Equipment H/W Testing Desk & Chair Setting

오디오 스튜디오

규    격    서

ITEM NO.	품명	수량
오-1	Digital Audio Mixing Console	1set

규격	세부사양	비고
세부규격	General 44.1–96kHz Internal Processing (Accumulator) 32bit (58bit) Total Mixing Ch 48 Bus 8 Aux 8 Internal Effects 4 Surround Effects 1 Internal GEQ (31 Bands) N/A Matrix (for Down Mix Recording & S/R) N/A Audio I/Os Analog Ch Inputs Total 20 Mic Preamp 16 XLR (A) 16 TRS (B) N/A Insert I/O 4 (OMNI IN) I/O Card Slot Mini-YGDAI 16CH I/O 2 2TR IN Analog TRS (+4dB) N/A RCA (-10dB) N/A 2TR IN Digital AES/EBU 1 COAXIAL 1 SRC Yes STEREO OUT Analog XLR (+4dB) OMNI OUT RCA (-10dB) N/A STEREO OUT Digital AES/EBU 1 COAXIAL 1 OMNI OUT XLR (+4dB) 12 TC INPUTS SMPTE (XLR) Yes MTC Yes WORD CLOCK Dimensions (H x D x W) 199 x 577 x 430 mm (7.8" x 22.7" x 16.9") Weight 19 kg (42 lbs) Same Brand Meter Bridge including Same Brand Wood Side Panel including	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
오-2	DA NLE Workstation	1set

규격	세부사양	비고
세부규격	Processor Two 2.8GHz Quad-Core Intel Xeon (8-core) Memory 2GB (2 x 1GB) HDD 320GB 7200-rpm Serial ATA 3GB/s Graphic ATI Radeon HD 2600 XT 256MB (Two dual-link DVI) ODD One 16x SuperDrive Apple Mighty Mouse Apple Keyboard Two FireWire 800 ports (one on front panel, one on back panel) Two FireWire 400 ports (one on front panel, one on back panel) Five USB 2.0 ports (two on front panel, three on back panel) Two USB 2.0 ports on included keyboard Front-panel headphone minijack and speaker Optical digital audio input and output TOSLINK ports Analog stereo line-level input and output minijacks PCI Express expansion Three open full-length PCI Express expansion slots One PCI Express 2.0 x16 slot Two PCI Express x4 slots All slots provide mechanical support for 16-lane cards 300W combined maximum for all PCI Express slots Software Mac OS X v10.5 Leopard (includes Time Machine, Quick Look, Spaces, Spotlight, Dashboard, Mail, iChat, Safari, Address Book, QuickTime, iCal, DVD Player, Photo Booth, Front Row, Xcode Developer Tools) iLife ’08 (includes iTunes, iPhoto, iMovie, iDVD, iWeb, and GarageBand) Size and weight Height: 20.1 inches (51.1 cm) Width: 8.1 inches (20.6 cm) Depth: 18.7 inches (47.5 cm) Weight (standard configuration): 42.4 pounds (19.2 kg)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
오-3	Multi Rec. S/W	1ea

규격	세부사양	비고
세부규격	Mic Inputs Line Outputs (1-8) Connector: Four balanced XLR jacks Mic Phantom Power: 48V Equivalent Input Noise: -129 dBu Frequency Response: +/- 0.1 dB, 20 Hz - 20 kHz Dynamic Range: 105 dB / 107 dB A-weighted THD + N: 0.0007% (-103 dB) Mic EIN: -129 dBu Input Sensitivity: +2.2 dBu Input Impedance: 2K Ohm Connector: Eight impedance balanced 1/4" jacks Frequency Response: +/- 0.5 dB, 20 Hz - 20 kHz Dynamic Range: 110 dB / 113 dB A-weighted THD + N: 0.0007% (-103 dB) Output Sensitivity: +18 dBu Supported Sample Rates: 44.1, 48, 88.2, 96 kHz Maximum Word Length: 24-bit S/PDIF: 2-channel optical or RCA jack pair Digital Optical: TOSLINK (ADAT, max 48 kHz sample rate) Word Clock: Two BNC jacks Host Connection: Two IEEE-1394a (FireWire) ports (6-pin-to-6-pin FireWire cable included) MIDI: 5-pin MIDI DIN connectors - one input, two outputs Size / Weight / Power Height: 2U rack (3.5 inches / 8.89 cm) Width: 19 inches / 48.26 cm Depth: 13.5 inches / 34.29 cm (including all knobs / connectors) Weight: 11.22 lbs / 5.09 kg Power Requirements: 100 - 240V, 50 - 60 Hz A/C (power cable included)

규    격    서

ITEM NO.	품명	수량
오-4	LCD Monitor	2ea

규격	세부사양	비고
세부규격	Viewable Size 19 inches Pixel Pitch 0.2835 mm Response Time (Typical) 5ms Viewing Angle 160 degrees Luminance (Brightness) 300 cd/m2 (Typical) Contrast Ratio 1000:1 Horizontal Scan Frequency kHz 30 kHz to 83 kHz (automatic) Vertical Scan Frequency Frequency kHz 56 Hz to 75 Hz (automatic), exception 1440 x 900 at 60 Hz Optimal Resolution 1440 x 900 at 60 Hz Preset Display Modes VESA, 720 x 400 – 31.5 kHz Horizontal, 70.0 Hz Vertical, 28.3 MHz VESA, 640 x 480 – 31.5 kHz Horizontal, 60.0 Hz Vertical, 25.2 MHz VESA, 640 x 480 – 37.5 kHz Horizontal, 75.0 Hz Vertical, 31.5 MHz VESA, 800 x 600 – 37.9 kHz Horizontal, 60.3 Hz Vertical, 49.5 MHz VESA, 800 x 600 – 46.9 kHz Horizontal, 75.0 Hz Vertical, 49.5 MHz VESA, 1024 x 768 – 48.4 kHz Horizontal, 60.0 Hz Vertical, 65.0 MHz VESA, 1024 x 768 – 60.0 kHz Horizontal, 75.0 Hz Vertical, 78.8 MHz VESA, 1152 x 864 – 67.5 kHz Horizontal, 75.0 Hz Vertical, 108 MHz VESA, 1280 x 800 – 61.6 kHz Horizontal, 59.81 Hz Vertical, 83.5 MHz VESA, 1280 x 1024 – 64.0 kHz Horizontal, 60.0 Hz Vertical, 135 MHz VESA, 1280 x 1024 – 80.0 kHz Horizontal, 75.0 Hz Vertical, 135 MHz VESA, 1440 x 900 – 55.9 kHz Horizontal, 60.0 Hz Vertical, 106.5 MHz Connector Type Analog, DVI-D (Digital) with HDCP Stand Tilt, Swivel, Height Adjustable, Pivot VESA Mounting Support Yes (100mm) Dimensions (Height x Width x Depth) 318.6 mm x 442.75 mm x 187.41 mm (13.3” x 17.43” x 7.38”) Weight (Monitor Only) 5.94 Kg (13.10 Ibs) AC input voltage 100 to 240 VAC / 60 or 50 Hz +/- 3 Hz / 1.5A Operating (Typical Maximum) Active Off - Less than 2W Switched Off - Less than 1W

규    격    서

ITEM NO.	품명	수량
오-5	Viewing Monitor	1ea

규격	세부사양	비고
세부규격	Ultra slim and light design New quiet fan-less design 852 x 480 resolution with 1.08 x 1.08mm pixel pitch Progressive display picture quality Picture-In-Picture source select 3D comb filter S-Video input Component video input terminals (Y,Pb,Pr) Computer input D-sub 15-pin High contrast high brightness panel 7 watt per channel built-in amplifier Audio: Output Power 7 watt per channel built-in amplifier Audio Decoder Dolby Pro-Logic Video: Display type 42" 16:9 Wide Screen Display Resolution 852 x 480 pixel count Connections: Composite video 1-RCA S-Video 1 Component Video 1 (Y,Pb,Pr) RGB 2 RS 232C 1 Audio 1 video, 1 component, 1 RGB Dimensions: 40 15/16"(W) x 25"(H) x 3 1/2"(D)

규    격    서

ITEM NO.	품명	수량
오-6	AV Option	1ea

규격	세부사양	비고
세부규격	SDI SDI stand AC adapter and power cable FireWire cable Using the Av CD-ROM Installation poster Input and output breakout cables for SDI, Component & Composite 2 adapters for S-Video connections Input and output audio cable adapters from mini-jack to RCA Size and Weight 6 3/4 " (17cm) wide by 11 1/4" (28.6cm) tall Only 1 inch (2.5cm) thick 1.5 lbs (.68 kg); 2.82 lbs (.1.28 kg) with stand

규    격    서

ITEM NO.	품명	수량
오-7	CDP	1ea

규격	세부사양	비고
세부규격	±12% pitch control for both CD and cassette XLR balance I/O GPI switches for remote control Independent operation for CD player Independent opertaion for Cassette deck Easy CD dubbing key A-B program function Continuous playback between CD and cassette Independent counter for each mechanism Shuffle playback function on CD player Repeat (single, ALl, A-B) playback on CD player Intro check on CD Programmable playback on CD Single playback on CD Delete program function on CD RTZ on cassette CPS (computomatic program search) on cassette

규    격    서

ITEM NO.	품명	수량
오-8	Midi Interface	1ea

규격	세부사양	비고
세부규격	Custom-designed VLSI technology Proprietary high-frequency phase engine Internal Power Supply (switchable 115V - 220V) 16x2 backlit LCD display 4 programmable front-panel knobs Status lights for MIDI IN/OUT, SMPTE and Networking 2 pedal inputs for continuous pedals or switch pedals Front panel MIDI IN and OUT ports Panic button 1 IEC power connector (115-220V) 2 SMPTE quarter-inch phone (+4/-10, hi-z) 2 pedal quarter-inch phone inputs (configurable for switch, continuous, or Alesis LRC) 1 Word Clock Out BNC TTL (1x or 256x) 1 Video In BNC 75-ohm terminated 1 USB port 1 Mac mini-DIN 8 serial 1 Mac/Network mini-DIN 8 serial 1 ADAT Sync Out 9-pin "D" 16 MIDI connectors

규    격    서

ITEM NO.	품명	수량
오-9	Reverb	1ea

규격	세부사양	비고
세부규격	Digital Inputs and Outputs Connectors RCA Phono (S/PDIF) Formats S/PDIF (24 bit), EIAJ CP-340, IEC 958 Output Dither HPF/TPDF dither 24/20/16/8 bit Sample Rates 44.1 kHz, 48 kHz Processing Delay 0.1 ms @ 48 kHz Frequency Response DIO DC to 23.9 kHz ± 0.01 dB @ 48 kHz Analog Inputs Connectors XLR, balanced Impedance, Bal / Unbal 21 kOhm / 13 kOhm Max. Input Level +24 dBu Min. Input Level for 0 dBFS 0 dBu A to D Conversion 24 bit, 128 x oversampling bitstream A to D Delay 0.65 ms / 0.70 ms @ 48 kHz / 44.1 kHz Analog Outputs Connectors XLR, balanced Impedance Balanced / Unbalanced 40 Ohm Max. Output Level +20 dBu (balanced) Output Ranges Balanced 20/14/8/2 dBu Unbalanced: 14/8/2 dBu D to A Conversion 24 bit, 128 x oversampling bitstream D to A Delay 0.63 ms / 0.68 ms @ 48 kHz / 44.1 kHz Dynamic Range 104 dB typ, 20 Hz to 20 kHz THD typ <-94 dB (0.002 %) @ 1 kHz, +20 dBu Output Frequency Response +0/-0.5 dB @ 48 kHz, 20 Hz to 20 kHz <-100 dB, 20 Hz to 20 kHz MIDI In/Out/Thru 5 Pin DIN Pedal 1/4" phone jack Finish Anodized aluminum front. Plated and painted steel chassis Display 23 character / 280 icon STN-LCD display Dimensions 19" x 1.75" x 8.2" (483 x 44 x 195 mm) Weight 4.1 lb. (1.85 kg) Mains Voltage 100 to 240 VAC, 50 to 60 Hz (auto-select) Power Consumption <15 W

규    격    서

ITEM NO.	품명	수량
오-10	Headphone Amp	1ea

규격	세부사양	비고
세부규격	Number of Channels 6 Input Connections Rear: 2 x XLR Female Main Inputs, Balanced 2 x 1/4" TRS Phone Main Inputs, Balanced Front:1 x 1/4" Stereo Phone Direct In 6 x 1/4" Stereo Phone Aux In Output Connectors Rear: 2 x XLR Male Main Outputs, Balanced 2 x 1/4" TRS Phone Main Outputs, Balanced 12 x 1/4" Stereo Headphone Outs* Front: 6 x 1/4" Stereo Headphone Outs 6 pairs labeled Headphone Out 1,2,3,4,5 and 6, wired in parallel with corresponding front panel Channels 1,2,3,4,5, and 6 Headphone Outs Maximum Output Level +21 dBm Function Controls 1 x Input Gain Knob 6 x Balance per Channel Knobs 6 x Output Gain per Channel Knobs 6 x Left Mute Switches(with Indicator) 6 x Right Mute Switches(with Indicator) 6 x Mono/Stereo Mode Switches(with Indicator) Frequency Response 10 Hz - 50 kHz, +/-3 dB THD + N 0.005% typ.@+4 dBu, 1 kHz, Gain 1 Noise >90 dB, unweighted, 22 Hz - 22 kHz(>95 dB @+4 dBu) Display 1 x 8-digit LED Meter Bars(Input) 6 x 4-digit LED Meter Bars(Output) -18/-12/-6/0/+6/+12/+18dbu/Clip -24/0/+12dBu/Clip Dimensions 19 x 8.5 x 1.7" (483 x 217 x 44mm) Weight 6.4 lb (2.9 kg) Specialties Dual Voltage Power Supply 3 Headphone Outputs per Channel Mono/Stereo Monitor Switching for each Channel

규    격    서

ITEM NO.	품명	수량
오-11	Condenser Mic.	1ea

규격	세부사양	비고
세부규격	Type: 1-inch large-diaphragm pressure gradient microphone Polar Pattern: Omnidirectional, wide cardioid, cardioid, hypercardioid, figure eight Frequency Range: 20 to 20,000 Hz Sensitivity: 23 mV/Pa (-33 dBV) ± 0.5 dB Maximum SPL: 200/400/800/1600 Pa = 140/146/152/158 dB SPL (0/-6/-12/-18 dB) (for 0.5% THD) Equivalent Noise Level (CCIR 468-2): 20 dB (0 dB preattenuation) Equivalent Noise Level: 6 dB-A (0 dB preattenuation) (DIN 45 412, A-weighted) Signal/Noise Ratio (A-weighted): 88 dB Preattenuation Pad: -6 dB, -12 dB, -18 dB, switchable Bass Cut Filter Slope: 12 dB/octave at 40 Hz and 80 Hz; 6 dB/octave at 160 Hz Impedance: <=200 ohms Recommended Load Impedance: >= 2,200 ohms Supply Voltage: 48 V phantom power to DIN/IEC Current Consumption: Approximately 4.5 mA Dynamic Range: 134 dB minimum Environment: Temperature Range: -10° C to +60° C (14° F to 140° F) Relative Humidity: 95% (+20° C/68° F), 85% (+60° C/140° F) Connector: 3-pin XLR to IEC Dimensions: 50 x 38 x 160 mm (2.0 x 1.5 x 6.3 in.) Net Weight: 300 g (10.6 oz.) Standard Accessories: H 85 shock mount, PF 80 pop screen, W 414 X dedicated foam windscreen, Sound Tool hard shell road case

규    격    서

ITEM NO.	품명	수량
오-12	Dynamic Mic.	2ea

규격	세부사양	비고
세부규격	Type Dynamic (moving coil) Frequency Response 50 to 15,000 Hz Polar Pattern Unidirectional (cardioid), rotationally symmetrical about microphone axis, uniform with frequency Sensitivity (at 1,000 Hz Open Circuit Voltage) -54.5 dBV/Pa (1.85 mV) 1 Pa = 94 dB SPL Impedance Rated impedance is 150 ohms (300 ohms actual) for connection to microphone inputs rated low impedance Polarity Positive pressure on diaphragm produces positive voltage on pin 2 with respect to pin 3 Connector Three-pin professional audio connector (male XLR type) Case Dark gray, enamel-painted, die cast metal; matte-finished, silver, spherical steel mesh grille Overall Dimensions See User Guide Net Weight 298 grams (10.5 oz)

규    격    서

ITEM NO.	품명	수량
오-13	Headphone	4ea

규격	세부사양	비고
세부규격	Analog Outputs 1/8" with 1/4" adapter Freq. Response 10Hz-20kHz Impedence 63 ohms Kind Closed Notes Circumaural design Weight 7.8 oz.

규    격    서

ITEM NO.	품명	수량
오-14	Mic Stand	3ea

규격	세부사양	비고
세부규격	Collapsible tripod boom stand Die-cast and steel construction Sleek black finish Ulta-light for easy transport

규    격    서

ITEM NO.	품명	수량
오-15	Synthesizer	1ea

규격	세부사양	비고
세부규격	Keyboard: 76-Key FSX Keyboard with Initial Touch and Aftertouch Polyphony: 128 Multitimbral: 16 Parts (Internal) Audio Input Parts (A/D, mLAN) Synthesis Method: AWM2 with Expanded Articulation Sequencer: 16-Track, 130,000 Note Sequencer Record and Playback: WAV, AIFF Controllers: 1 x Pitch Wheel 1 x Modulation Wheel 1 x Ribbon Controller 8 x Assignable Sliders 8 x Assignable Knobs 2 x Assignable Function Buttons 1 x Data Dial Inputs/Outputs: 1 x AC Power Input 1 x Ethernet Connector 1 x USB to Host Connector 1 x USB to Device Connector 1 x S/PDIF RCA Coaxial Digital Output 3 x MIDI Connectors (In, Out, Thru) 2 x Footswitch Jacks 2 x Foot Controller Jacks 2 x 1/4" Stereo Outputs (4 Jacks, 2 Assignable) 1 x 1/4" Headphone Output 1 x 1/4" Stereo Input (2 Jacks) Storage: Internal Memory Up to 1GB of Optional Sample RAM Display: 320 x 240 Graphic Color Backlit LCD with Adjustable Contrast Dimensions (WxDxH): 49.3 x 15.4 x 4.8" (1252 x 391 x 122mm) Weight: 37.5 lbs (17kg)

규    격    서

ITEM NO.	품명	수량
오-16	Monitoring Speaker	2ea

규격	세부사양	비고
세부규격	Components, LF: 6.5" cone Components, HF: 1.0" Titanium dome Enclosure, Type: Bass-Reflex Enclosure, Material: PP Amplifier Specifications: Output Power, LF: 80 W, THD = 0.05 %, RL = 4 ohms Output Power, HF 50 W, THD = 0.05 %, RL = 6 ohms S/N, IHF-A filter: > 99 dB, LEVEL = Max Input Sensitivity, XLR-3-31: +4 dBu, LEVEL=Center, -6 dBu, LEVEL=Max Input Connectors, Impedance: XLR-3-31 (balanced), 10 k ohm LEVEL control: 31 Positions Detent type VR (Min = -8 Attenuation) LOW CUT switch: FLAT/80 Hz (12 dB/oct) / 100 Hz (12 dB/oct) HIGH TRIM: +1.5/0/-1.5 dB at 15 kHz LOW TRIM: +1.5/0/-1.5/-3 dB at 45 Hz POWER SWITCH: on/off Indicators: Green LED Power On, RED LED Clipping Power Consumption: 100 W General Specifications: Type: Biamp 2-way Powered Speaker Crossover Frequency: 2.5 kHz, LF: 30dB/oct, HF: 30dB/oct Overall Frequency Response: 45 Hz - 40 kHz (-10 dB) Maximum Output Level: 106 dB, 1 m on Axis Magnetic Shielding: Yes Dimensions (W x H x D): 218 x 330 x 235 mm Weight: 12.2 kg

규    격    서

ITEM NO.	품명	수량
오-17	Music Accompaniment Machine	1ea

규격	세부사양	비고
세부규격	Type : Karaoke HDD : 250GB Voltage : AC 110V ~ 220V Watt : 32W Weight : 6kg Size : 420 x 150 x 287 Frequency : 20Hz ~ 20KHz Output : 2Vp-p Distortion : 0.05% S/N : 70dB(1KHz) Composite : 1.0Vp-p(75ohm) Monitor : 1.0Vp-p(75ohm) Component : Y = 1.0 Vp-p Pb = 0.7 Vp-p Pr = 0.7 Vp-p TV : NTSC * 납품 시점의 최신 곡 수록

규    격    서

ITEM NO.	품명	수량
오-18	Audio Rack Desk w/ Chair	1set

규격	세부사양	비고
세부규격	Desk : End Panels to Mahogany Hardwood Single Monitor Arm (black or silver) Rack Inserts can be exchanged for monitor inserts Add locking CASTERS to your console. (Raises console 3”) BLANK PANELS L.M. Powder coated 14g steel panels 2 space panel: $12.50 RACK RAIL SCREWS Black Oxide, phillips truss head rack-rail screws. 10-32”x3/4” Dimension : 29" 41" 50" 11" 15" 10" Chair : Unupholstered back and seat in graphite color Graphite cololr base and frame 2 1/2" Black casters Standard Height, Standard Tilt Fixed Arms-Black-No upholstery

규    격    서

ITEM NO.	품명	수량
오-19	Sub Desk Rack	1set

규격	세부사양	비고
세부규격	Panels to Mahogany Hardwood End Panels to Platinum Powdercoat BLANK PANELS L.M. Powder coated 14g steel panels 2 space panel: $12.50 RACK RAIL SCREWS Black Oxide, phillips truss head rack-rail screws 10-32”x3/4” with #10 nylon washer

규    격    서

ITEM NO.	품명	수량
오-20	Wall Panel	1ea

규격	세부사양	비고
세부규격	제작사양 : XLR Audio In : 8 XLR Audio out : 4 RCA Audio In/Out : 2 pairs BNC In/Out : 2 pairs

규    격    서

ITEM NO.	품명	수량
오-21	Audio Patch Bay	1ea

규격	세부사양	비고
세부규격	Audio Bantam (TT); 2x48; 2RU; Black 12" Chassis; Over/Under Designation Strips; Mono Spacing; Full-Normal, Isolated Grounds; E3 Rear Interface. Jacks rated to 30,000 minimum insertion cycles Copper-nickel-silver alloy leaf springs with gold-plated cross bar switching contacts and nickel-plated sleeve bushings Precision-stamped reinforced steel jack frame Gold-plated contacts used in E3, E56 and E90 rear interface Wired with low-capacitance, AES/EBU-rated shielded, twisted pair Large user-friendly designation strips Panels made from 3/16" solid aluminum with a durable powder-coat finish Mating connectors, contacts and normals (where applicable) are included with all standard rear interfaces Normals and grounding for individual circuits can be easily changed by the end-user Programming shunts located under designation strips Normaling shunts are placed vertically and Grounding shunts are placed horizontall Low Capacitance Flexible 110 Ohm digital cabling AES compatible Electroless nickel-plating for added durability *50cm Bantom Patchcord x 10ea 포함

규    격    서

ITEM NO.	품명	수량
오-22	Tally Controller	1ea

규격	세부사양	비고
세부규격	Channel status LEDs Dry contact or voltage control inputs Dry contact or voltage control outputs On air & speaker mute control 19″1 Rack unit type Tally Input : 10ch Control Output : 8ch On Air / Mute Control Output : 2ch Power : AC 85V ~ 264V , 50/60 Hz Dimensions : 483 x 44 x 350

규    격    서

ITEM NO.	품명	수량
오-23	On-Air Lamp	3ea

규격	세부사양	비고
세부규격	On Air display lamp : Red LED type Tally Input : under 10mA Power : 110 / 220 Volts , AC 60Hz, 2W Dimensions : 270 x 78 x 60

규    격    서

ITEM NO.	품명	수량
오-24	Install & Materials	1lot

규격	세부사양	비고
세부규격	- Equipment Setting - Cable Connecting - Cable Wiring - S/W Installation - Warranty Service - Hiding Cable - Fixing Equipment - S/W Installment/Testing - H/W Testing - Desk & Chair Setting

장비 대여실

규    격    서

ITEM NO.	품명	수량
장-1	Digital Camcorder 1	2set

규격	세부사양	비고
세부규격	Carl Zeiss Vario-Sonnar T* zoom lens, 12x (optical), f = 4.4 to 52.8 mm, f = 32.0 to 384 mm* at 16:9 mode, f = 39.5 to 474 mm* at 4:3 mode, filter diameter: 72 mm - Built-in filter Clear, 1/4, 1/16, 1/64 - Imaging system 1/3-inch, progressive 3 ClearVid CMOS Sensor system with Exmor technology - Picture elements Approx. 1,037,000 pixels, 1,120,000 pixels - Focus Auto,manual (focus ring/one push auto/infinity/AF assist) - White balance Auto, one-push auto (A/B positions), indoor (3200 K), outdoor (selectable level -7 to +7, approx. 500K/step), manual WB Temp (selectable 2300K to 15000K, 100K/step) - Manual shutter speed Auto: 1/50 - 1/1750 - Manual: 50i/25p: 1/3 - 1/10000 - Gain -6, -3, 0 , 3, 6, 9, 12, 15, 18, 21 dB - Minimum illumination 1.5 lux (auto gain, auto iris, 1/25 shutter) - Recording format HDV1080/50i, DVCAM, DV SP 576/50i (PAL) Play out/Down conversion format HDV1080/50i, DV SP 576/50i - Playback/Rec time HDV/DV SP: Max. 63 min with PHDVM-63DM - DVCAM: Max. 41 min with PHDVM-63DM cassette - Audio/Video output 10-pin connector A/V OUT jack (composite, unbalanced audio x2ch with the supplied cable) - Component video output Component out jack (special connector) - HDV/DV input/output i.LINK interface (IEEE 1394, 6-pin) - XLR audio input XLR 3-pin female x 2ch - Headphone Stereo mini jack (ø3.5 mm) - LANC Stereo mini-mini jack (ø2.5 mm) - Digital video output HDMI connector - LCD view finder 0.45-inch type (Viewable area measured diagonally), approx. 1,226,880 dots (852x480x3[RGB]), 16:9 ratio - LCD monitor 3.2-inch type (Viewable area measured diagonally), XtraFine LCD, approx. 921,600 dots, hybrid type, 16:9 ratio with NP-F970 Battery x each 1ea (total 2ea) UV Filter x each 1ea (total 2ea) VQ1050D Charger x 1ea (total 1ea) 2 steps Carrying hard case x each 1ea (total 2ea)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
장-2	Digital Camcorder 2	8set

규격	세부사양	비고
세부규격	HDV camcorder provides real 1080i HD acquisition superb image quality and comprehensive functionality for professional use, in a handy camcorder form factor. expand the adoption of HDV and lead the entry level HD market by providing a compact and low cost solution. 1/3 inch C-MOS imager. 920x1080 native imager is also capable of 3 mega-pixel still images. Combined with a high quality Optical Zoom Carl Zeiss Vario-Sonnar T* Lens new 14 bit A/D and DXP digital Extended Processor, records this exceptional imagery using the recently adopted HDV 1080i format onto a DVCAM mini cassette. Recording Format : HDV Recording System : NTSC Optical Zoom : 10x LCD Panel Size : 2.7 in. Optical Zoom : 10x · Lens Focal Length : 41 - 410 mm Filter Diameter : 37 mm Video Modes : SP · Image Stabilizer : Digital Image Stabilizer Low Lux : 7 Lux Memory Card Type : Memory Stick Duo · Digital Still Shot Mode : Still Shot Capability · MPEG Movie Mode : MPEG Movie Mode Output Interfaces : Composite (Video),· Audio (RCA),· FireWire / DV / i.Link,· USB,· Headphones Jack Input Interfaces : Audio (RCA) · FireWire / DV / iLink Microphone Type : External/Optional Installed with MP-QM91 Large Battery x each 1ea (total 8ea) UV Filter x each 1ea (total 8ea) Wide converter Lens x 2ea (total 2ea) AC-VQ50 Charger x 4ea (total 4ea) Carrying hard case x each 1ea (total 8ea)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
장-3	Digital Camcorder 3	11set

규격	세부사양	비고
세부규격	Weights and Measurements Weight (Approx.) : 13 oz (380g) with suppied battery Dimensions (Approx.) : 2 7/8" x 2 7/8" x 4 5/8" (73 x 71 x 115mm) General Imaging Device : 1/6" Advanced HAD™ CCD Pixel Gross : 680K Recording Media : 30GB5 Hard Disk Drive, Memory Stick PRO Duo™ Media (sold separately) Recording and Playback Times : HQ: up to 7 hours, SP: up to 10 hours, LP: up to 20 hours Video Actual : 260K Pixels Still Actual : 340K Pixels Optics/Lens 35mm Equivalent : 39-1560mm (16:9 Camera Mode), 36-1440mm (4:3 Camera Mode), 36-1440mm (4:3 Memory Mode) Aperture : f1.8-4.1 Exposure : Touch Panel (32 steps) Filter Diameter : 30mm Focal Distance : 1.9-76mm; Telemacro Mode - 430mm Focus : Full Range Auto/Manual (Touch Panel) Progressive Shutter Mode : N/A Shutter Speed : Auto, 1/60-1/4000 (Scene Selection Mode) Optical Zoom : 40X Digital Zoom : 2000X Display LCD Screen : 2.5" Touch Panel SwivelScreen™ LCD Display (123K Pixels) with NP91 Large Battery x each 1ea (total 11ea) Carrying soft case x each 1ea (total 11ea)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
장-4	Tripod	2set

규격	세부사양	비고
세부규격	1. Fluid Head Tilt : +90 - 60 Pan : 360 Sliding Quick Realease Plate : 3/8" and 1/4" camera screw Sliding Travel of Plate : 58mm 2. Tripod Max : 15kg Length : 32 ~ 156 Fixed : 71 Ball : 75mm 3. 75mm Half Ball 4. Carrying Bag Closed length: 87.0 cm Minimum height: 42.5 cm Maximum height: 166.5 cm Legs: 3 section Weight: 5.5kg Load capacity: 8kg with Portable Dolly x each 1ea (total 2ea)

규    격    서

ITEM NO.	품명	수량
장-5	Tripod 2	8ea

규격	세부사양	비고
세부규격	Max. height: 1550mm Min. height: 755mm Legs: 3 section Ball Base: 75mm Weight: 3.5kg Max. camera weight: 5kg

규    격    서

ITEM NO.	품명	수량
장-6	Digital Still Camera(DSLR)	2ea

규격	세부사양	비고
세부규격	Sensor resolution 12.2 megapixels Optical sensor type CMOS Effective sensor resolution 12,200,000 pixels Gross sensor resolution 12,400,000 pixels Light sensitivity ISO 100-1,600 Shooting programs Landscape, Portrait mode, Night portrait, Sports mode, Close-up Special effects Landscape, Portrait, Faithful, Neutral, Monochrome Max shutter speed 1/4000 s Min shutter speed 30 s Continuous shooting speed 3.5 fps Exposure metering Spot (4%), Centre-weighted, Partial (9%) Exposure modes Aperture-priority, Depth-of-field, Bulb, Automatic, Program, Shutter-priority, E-TTL II program flash, Manual Exposure compensation ±2 EV range, in 1/2 or 1/3 EV steps Auto exposure bracketing 3 steps in 1/2 or 1/3 EV steps White balance Custom, Automatic, Presets Still image format RAW + JPEG, JPEG, RAW Auto focus TTL phase detection Lens type Zoom Focal length 18-55 mm Equivalent 35mm focal length 29-88 mm Focus adjustment Automatic, Manual Focus zones 9 Min focus range 249 mm Lens aperture F/3.5-5.6 Optical zoom 3 x Zoom adjustment Manual Viewfinder type Optical Display type LCD Display size 76 mm Display resolution 230,000 pixels Expansion slots SD Memory Card Size (W x H x D) 130 x 99 x 61 mm Weight 476 g with EF-S18-55mm Lens x each 1ea (total 2ea) LP-E5 Spare Battery x each 1ea (total 2ea) SDMemory 4GB x each 1ea (total 2ea) Carrying Soft Case x each 1ea (total 2ea)

규    격    서

ITEM NO.	품명	수량
장-7	Wide Single Lens	1ea

규격	세부사양	비고
세부규격	Fullframe Coverage YES Field of View (degrees) [See Comments section below] Focal Length Prime 15 mm (APS-C 35mm equiv = 24 mm) Aperture Range Prime f2.8 - f22 Motor AFD Elements/Groups 8/7 Close Focus 0.2 m : 0.7 ft Maximum Magnification 0.14x Length/Diameter 2.4"/2.4" : 61 mm / 61 mm Weight 11.7 oz : 332.3 gm Filter rear gel Lens Hood Built-in

규    격    서

ITEM NO.	품명	수량
장-8	Zoom Lens	1ea

규격	세부사양	비고
세부규격	Fullframe Coverage YES Field of View (degrees) Horizontal,Vertical, Diagonal Full Frame - 36x24mm APS-C - 22.5x15mm Full Frame Wide : H - 28.8 : V - 19.5 : D - 34.4 Full Frame Tele : H - 10.3 : V - 6.9 : D - 12.3 APS-C Wide : H - 18.3 : V - 12.2 : D - 21.9 APS-C Tele : H - 6.4 : V - 4.3 : D - 7.7 Min Focal Length 70 mm (APS-C 35mm equiv = 112 mm) Max Focal Length 200 mm (APS-C 35mm equiv = 320 mm) Max Aperture (Wide-Tele) f4 - f4 Min Aperture (Wide-Tele) f32 - f32 Image Stabilization 3 stops Motor USM Elements/Groups 16/13 Close Focus 1.2 m : 3.9 ft Length/Diameter 6.8"/3" : 172.7 mm / 76.2 mm Weight 25 oz : 710 gm Filter 67

규    격    서

ITEM NO.	품명	수량
장-9	Digital Camera	21set

규격	세부사양	비고
세부규격	6 Megapixel CCD imager for up to poster size prints 4x optical 35-140mm f/2.6-5.5 zoom, 4x digital zoom 2.5" color LCD with up to 10x playback zoom Advanced TTL AiAF 9-point autofocus system Program AE, Shutter-speed priority, Aperture priority and Manual modes Pre-programmed creative scene modes for beginners Movie mode w/sound, 640x480 / 320x240 up to 1GB, 160x120 up to 3 minutes 2.3fps Continuous burst capture of Large/Fine images Evaluative metering on focus point, Center-weighted or Spot options Stitch Assist mode for perfect panoramas Exposure compensation: +/-2EV in 1/3-step increments White Balance: Auto, 5 presets or Custom Orientation sensor that automatically detects vertical or horizontal shooting Low-light focus assist illuminator Light-guide zoom flash, angle changes with focal length Optional High-Power Flash HF-DC1 Shutter speeds of 15 seconds to 1/2000 second Selectable ISO settings from 80 to 800 Voice memo (up to 60 secs) can be attached to images Built-in microphone and speaker Powered by two standard AA type batteries Direct print and PictBridge Compatible USB 2.0 high speed connectivity for PC and Mac Secure Digital memory cards, 16MB supplied 1GB SD Memory Rechargeable set 2in Carrying soft case including

규    격    서

ITEM NO.	품명	수량
장-10	Two Way Light	6ea

규격	세부사양	비고
세부규격	GE SEALED BEAM ALL GLASS LAMP 2개(옵션선택) + 본체 + Stand 몸체 색상 : 블랙 정격 전압 : 220 V 소비 전력 : 1,300W 점등 방법 : 스위치 방식 사용 램프 : GE 120V with DWE Lamp x 6ea FBE Lamp x 6ea Carrying Case x 2ea

규    격    서

ITEM NO.	품명	수량
장-11	Video Light	2ea

규격	세부사양	비고
세부규격	Lamp Type LED Daylight Balanced 5500K Mount Type Shoe Mount Power Source Sony L Series Lithium Batteries Power Consumption 16W Power Connector Specific to L Series Batteries Dimensions (WxDxH) 4 3/8 x 6 x 5 1/8" 10.8 x 12.9 x 15cm Weight 14.9 oz 420 g

규    격    서

ITEM NO.	품명	수량
장-12	Reflector	5ea

규격	세부사양	비고
세부규격	Light Reflector 82cm White & Silver Type 원형 강선 와이어 내장으로 자동 펼쳐짐 Including Soft Case

규    격    서

ITEM NO.	품명	수량
장-13	Gelatine	1roll

규격	세부사양	비고
세부규격	Lee Filters 25'x48" Flame Red Lighting Filter Creates fire effect. Roll - 7.62m x 1.22m (25' x 48") Lee Filters 25'x48" No Colour Blue Lighting Filter Converts tungsten to Moonlight for green seas, cycloramas with 147 to produce sunsets Lee Filters 20"x24" Dark Green Lighting Filter Cycloramas - good for back lighting

규    격    서

ITEM NO.	품명	수량
장-14	Location Sound System	1sys

규격	세부사양	비고
세부규격	1. Headphone Rugged Design: Proven to be reliable in the toughest situations Folding Construction: Compactness in storage 40mm Driver Unit: For clear, high quality sound reproduction Closed-Ear Design: Comfort and reduction of external noise interference Stereo Unimatch Plug: 1/4" and 1/8" applications Gold Connectors and OFC Cord: Reliable and stable signal connection and transmission Supplied Soft Case: Protective storage Rugged Design Folding Construction 40mm Driver Unit Closed-Ear Design Stereo Unimatch Plug Gold Connectors and OFC Cord Supplied Soft Case Headphone type: Sealed-ear, dynamic Frequency response: 10-20kHz Driver size: 40mm Plug-type: Stereo Unimatch plug 1/4" and 1/8" 2. Boom pole with carrying case Aluminium boom length 93-320cm weight 800g thread 3/8" Carrying Case 3. Location Mic Pick-up pattern super-cardioid/lobar Sensitivity in free field, no load (1kHz) 50 mV/Pa +- 2,5 dB Nominal impedance 200 Ohm (K6) Min. terminating impedance 1000 Ohm ( K6) Equivalent noise level 10 dB	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
장-14	Location Sound System	1sys

규격	세부사양	비고
세부규격	Equivalent noise level weighted as per CCIR 468-3 21 dB Dimensions d 22,5 x 221 mm Nominal impedance 200 Ohm Min. terminating impedance 1000 Ohm Output voltage 2 V Power supply Phantom 12 - 48 V 1x Typ IEC LR 06 Current consumption 2,2 mA Operating time (Battery) max. 150 h Dimensions d 22 x 94 mm (netto) Weight ca. 45 g Gain : 0 dB 4. Suspension pistol grip Required for mounting in MZW "blimp" windscreen. May be boom or stand mounted. Requires MZA-216 adapter (included). Includes interchangeable mike clips for MKH-416/MKH-816, or MKH-20 through MKH-70 5. Hairy cover Long hair wind muffs greatly reduce high velocity wind-noise when used with MZW series blimp windshields and MZS-20-1 pistol grip/shock mount. Requires MZW 20-1 "blimp" windscreen. 6. Bascket wind shield Blimp windshield for MKH-20/30/40/50. (Requires MZS20-1) 7. Carrying aluminum box Aluminum Carrying Case for Location System 8. Cable 10m M/F XLR connected cable * 1ea	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
장-15	Audio Recorder	1set

규격	세부사양	비고
세부규격	Stereo recording to CF Memory media 44.1kHz to 192kHz recording resolution at 16- or 24-bit Time-stamped Broadcast WAVE file format is easily imported into DAW software and spotted into projects with sample accuracy Retake button allows user to re-do last recording with a single button press Audio files continually re-saved to safeguard against data loss Comprehensive system and transport control from the front panel or a PS/2 keyboard XLR mic inputs with phantom power and analog peak limiter Unbalanced stereo RCA I/O/PDIF digital I/O Headphone output Built-in mono microphone and speaker for desktop interview applications Analog level controls for easy operation without the need to look at the unit FireWire interface for fast data transfer to a computer SMPTE/LTC timecode input on locking XLR balanced jack Timestamps Broadcast WAVE recordings from SMPTE input Chase locks to incoming SMPTE timecode Video clock input resolves to house clock Tri-level sync support for HDTV applications Includes Frame Lock, Lock and Release and flexible Freewheel settings for unpredictable timecode sources Pull-up and Pull-down sample rates included for video format compatibility Familiar tape machine-style layout and function Angled screen for table-top or shoulder strap use Large, uncluttered LCD display Shortcut keys and LED indicators for frequently-accessed functions Recessed Compact Flash slot Runs on (8) readily available AA batteries or DC power adapter Approximately 5.5 hours of operating time on battery power * Including Field Case(CS-P2), AC Adapter

규    격    서

ITEM NO.	품명	수량
장-16	Other Equipments for Recording	5set

규격	세부사양	비고
세부규격	1. XLR Adoptor Input Connections 2 x XLR Female, Balanced 1 x 1/8" Mini Jack(Left), Unbalanced Output Connectors 1 x 1/8" Stereo Mini Plug on 10" Cable, Unbalanced Input Impedance Mic: Nominal 200 ohms (low impedence) Line: 100k ohms Gain Adjustable from unity to zero in 10 steps Maximum Input Voltage Mic: 880mV Line: 10V (1%THD@60Hz) Attenuation / Gain Approx. -50db Ripple -1db (20 hz -20khz) Dimensions 3.25 x 2.5 x 1.25"(in.) Weight 10 oz 2. Boom pole with carrying case Aluminium boom length 93-320cm weight 800g thread 3/8" Carrying Case 3. Location Mic Direction pattern : Super-Cardioid Frequency : 18 Hz ~ 20kHz HPF Output impedence : 50 Ohm S/N : -36dB Maximum SPL : 139dB Power Supply : P48 Phamtom 1.5V AA 4. Cable 10m M/F XLR connected cable * 1ea 5. Voice Recorder Rec. Time : Max 595 Hours Quality : 96kbps Rec. Source : Int. Mic / Ext. Mic, Phone, Aux Format : ZVR, MP3, Wma Battery : Litum 3.7V PC : USB 1.1 Battery life : Max 8 Hours Pin Mic 포함	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
장-17	Film Slate	5set

규격	세부사양	비고
세부규격	STANDARD Size 9.5" X 11" (23cmX28cm) 재질 : 아크릴

규    격    서

ITEM NO.	품명	수량
장-18	Carrier	2ea

규격	세부사양	비고
세부규격	카트크기 : 61cm x 90cm 바퀴소재 : 우레탄 접이식 카트 Dolly : 4ea Handle : O Color : Green

규    격    서

ITEM NO.	품명	수량
장-19	Rain Cover	2ea

규격	세부사양	비고
세부규격	Quick easy set-up with pull tight cords and Velcro all along the rim for quick access and closure and full size window to monitor all controls when working. Adjustable lens hood to fit smallest lens up to biggest wide angle lenses or mattbox Flexible view finder sleeve Comfortable cone shaped opening is roomy when camcorder is hand-held Quick easy set-up even when mounted on tripod Adjustable straps for perfect fit Velcro top opening for: connection for SPS light hood, two movable sleeves, connection for 5" VF hood Dimensions (L x H): 76cm x 31 cm Weight: 0.45kg, 0.99lbs

규    격    서

ITEM NO.	품명	수량
장-20	Portable DV Deck	2ea

규격	세부사양	비고
세부규격	Width 7.9 in Depth 6.4 in Height 2.5 in Weight 2.9 lbs Sound Output Mode Stereo Type Digital VCR Media Format NTSC Video Head Qty 2 Playback Speed LP, SP Recording Speed LP, SP Media Type Mini DV Remote Control Remote control - Infrared Type Remote control Technology Infrared Connector Type 1 x IEEE 1394 (FireWire/i.LINK) ( 4 pin FireWire ), 1 x USB, 1 x Composite video/audio input ( RCA phono x 3 ), 1 x S-Video input ( 4 pin mini-DIN ), 1 x Headphones ( Mini-phone stereo 3.5 mm ), 1 x Composite video/audio output, 1, 1 ( 19 pin HDMI Type A ), 1 x S-Video output Slot Provided 1 Antenna None Cables Included A/V cable Power Device Power adapter - External Type External

규    격    서

ITEM NO.	품명	수량
장-21	Wacky Talky	8ea

규격	세부사양	비고
세부규격	채널수 : 25채널(38CTCSS) 주파수범위 : 448.7500 ~ 449.2625MHz 출력 : 0.5W 크기 : 184(높이) × 64(가로) × 31(두께)mm 무게 : 140g 구성품 : 본체, 설명서, 벨트크립, 배터리, 충전기 생활방수기능 디지털 나침반 기능 FM Radio 기능 진동 호출 기능 디지털온도계 기능 온도경보 설정 기능 스톱워치 기능 Arlam(시계) 기능 Scrambler(비밀통화) 기능 차량에서 충전하면서 사용가능 Roger Beep 기능

규    격    서

ITEM NO.	품명	수량
장-22	W/L Mic.	10ea

규격	세부사양	비고
세부규격	1. Reciever Operating Frequency 740.250 ~ 751.750 ㎒ Frequency Stability ± 15 PPM Receiver Sensitivity 3 ㎶ Audio Frequency Response 60㎐ ~ 15㎑ (±3dB) Signal to-Noise Ratio More than 90dB Maximum FM Deviation 56K Harmonic Distortion 0.6% Audio Frequency Output - 20dBm ~ -10dBm (ADJ.) Squelch 0 ~ 30㎶ (ADJ.) Pre-scaled channel 16CH Antenna Type WHIP ANT Operating Time 5 Hours Power Supply DC 3V (AA" 1.5 × 2) Dimension (W x H x D) 63 × 107 × 19 (㎜) Weight 100g (Without Batteries) 2. Transmitter Operating Frequency 740.125 ~ 751.875 ㎒ RF OUTPUT 10㎽ Audio Frequency Response (RX + TX) 60㎐ ~ 15㎑ (±3dB) Frequency Stability ± 15 PPM Signal to-Noise Ratio (RX + TX) More than 90dB Modulation PLL Synthesizer Harmonic Distortion (RX + TX) 1K 0.6% Pre-scaled channel 16 Channels Antenna Type WHIP ANT Operating Distance 100m Operating Time 6 Hours Power Supply DC 2.4V (AA" 1.2 × 2) Dimension (W x H x D) 62.6 × 96.3 × 18.5 (㎜) Weight 100g (Without Batteries)

규    격    서

ITEM NO.	품명	수량
장-23	Steady Cam	1ea

규격	세부사양	비고
세부규격	MICC1 - Standard type Microphone clip MICC2 - Universal spring type microphone clip MICC4 - Universal Shock Mount Microphone Holder 595cla - Clamp specifically designed for the Fig Rig

규    격    서

ITEM NO.	품명	수량
장-24	Wheelchair Tripod	5ea

규격	세부사양	비고
세부규격	Wheelchair Mount with Fluid Tripod Head Base Clamp Section: Weight: 2 lbs Size: 5.75 x 1.50 x 2.0 Material: Aluminum L-Tube: Weight: 1 lbs Size: 15 x 22 (L Shaped .75 tube) Material Steel (plated smooth) Camera Base/Tripod Mount: Weight: 1 lbs Size: 6.0x 2.7 x 1.0 Material: Aluminum Pan-Tilt Base Mount: Weight: 1 lbs Size: 6.0 x 2.7 x 1.5 LTM-WPCT Production Control Center: For LTM-M1 Pan-Tilt Section: Power Source: 4 AA batteries Vertical Tilt Angle: 5Maximum Horizontal Pan Angle: 0Maximum Maximum Speed- Vertical: 2.4 deg/second Maximum Speed-Horizontal: 8.0 deg/second Maximum Camera Weight: 6 Pounds (2.7 kg) Size (without platform): 145mm x 115mm x 103mm Weight (without batteries): 28 oz(800gm) Lan-C Section: Power Source: Provided by Camera Plug: 2.5mm Stereo Mini - LAN-C Cable: Length: 11.8-78(coiled) General: Operating Temperature: 0 deg C to 40 deg C Size: 3.5" L x 3.5" H x .75" W Motorized Panhead Version: Automatic or remote controlled movement up to 90 degrees left or right from 0 degrees position and 15 degrees panhead tilt. High quality unit consists of motorized panhead and remote control

규    격    서

ITEM NO.	품명	수량
장-25	I-Type office desk / chair	1ea

규격	세부사양	비고
세부규격	책상 크기 : 1600*1200*750 책상 : 우드 월 넷, “L” 형 의자 : 편안하고 인체공학적인 사무용 의자 색상 및 세부 규격은 협의 후 결정

규    격    서

ITEM NO.	품명	수량
장-26	NLE NoteBook	6ea

규격	세부사양	비고
세부규격	SYSTEM COLOR Jet Black edit PROCESSOR Intel® Core™ 2 Duo T8300 (2.4GHz/800Mhz FSB/3MB cache) OPERATING SYSTEM Genuine Windows Vista® Home Edition DISPLAY high contrast, widescreen 17.0 inch display (1440 x 900) VIDEO CARD 128MB NVIDIA® GeForce® 8400M GS MEMORY 2GB Shared Dual Channel DDR2 at 667MHz HARD DRIVE Size: 320GB SATA Hard Drive (5400RPM) OPTICAL DRIVE CD / DVD writer (DVD+/-RW Drive) WIRELESS NETWORK CARDS Intel Next-Gen Wireless INTEGRATED WEBCAM No Webcam Option BATTERY OPTIONS 56Whr Lithium Ion Battery (6 cell) SOUND OPTIONS High Definition Audio 2.0 My Software & Accessories ANTIVIRUS SOFTWARE McAfee SecurityCenter with anti-virus, anti-spyware, firewall, 24-months OFFICE SOFTWARE No Productivity software pre-installed WARRANTY AND SERVICE 2Yr In-Home Service, Parts + Labor, 24x7 Phone Support DATASAFE ONLINE BACKUP Included 3 GB DataSafe Online Backup for 1Yr DIAL-UP INTERNET ACCESS 6 Months FREE EarthLink Internet Access Network Card Integrated 10/100 Network Card and Modem Adobe Software Adobe® Acrobat® Reader 8.1 Labels Windows Vista™ Premium Processor Branding Intel Centrino Core Duo Processor DOMS Camera Mod Basic Black Matte LCD back color w/o Camera PHOTO AND MUSIC SOFTWARE No Entertainment software pre-installed

규    격    서

ITEM NO.	품명	수량
장-27	DLP Projector	2set

규격	세부사양	비고
세부규격	System DLP® Projection system Device 0.7" (diagonal) DLP® chip 4:3 Pixels 786,432 (1,024 x 768) x 1 total of 786,432 pixels Lamp 210 W UHM™ lamp x 2 (Dual Lamp System) Brightness (normal lamp)*1 4,000 lumens (dual lamp, high power) Contrast ratio*1 1,600:1 (full on/full off, contrast mode: high) Resolution 1,024 x 768 pixels Lens Powered zoom/focus lens, Supplied lens: (1.8-2.4:1) F = 1.7-2.0, f = 25.6-33.8 mm Screen size 50 - 600 inches Lens shift Vertical (powered), horizontal (manual) RGB input scanning frequency fH 15-91 kHz, fv 50-85 Hz Dot clock 150 MHz or lower Component signal 480i, 480p, 576p, 720/60p, 720/50p, 1080/60i, 1080/60p 1080/50i, 1080/50p Video signal NTSC, NTSC4.43, PAL, SECAM Terminals VIDEO IN BNC S-VIDEO IN Mini DIN 4-pin RGB1/YPBPR IN BNC x 5 RGB2 IN D-sub HD 15-pin DVI-D IN 24pin DVI 1.0 compliant, HDCP for single link RS-232C IN D-sub 9-pin female RS-232C OUT D-sub 9-pin male REMOTE 1 IN M3 jack REMOTE 1 OUT M3 jack REMOTE 2 IN D-sub 9-pin female (parallel) LAN RJ-45x1 with PJLink™ (class 1), 10Base-T/100Base-TX Keystone correction range ±30° (with standard lens) Installation Front/rear, ceiling/floor Power cord length 9.10' (3.0m) Power supply 220-240 V AC, 50 / 60 Hz Power consumption 520 W (570 VA) Dimensions (W x H x D) (530 x 167 x 441 mm) Weight 30.2 lbs (13.7 kg) with supplied lens Operating temperature 32 -113 °F (0 -45 °C) Operating humidity 20-80% (no condensation) with Carrying Hard Case 제작사양 x each 1ea (total 2ea)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
장-28	Portable Film Screen	2ea

규격	세부사양	비고
세부규격	유압식 필름스크린 사이즈 : 80“(180 x 180cm) 후면이 X 구조로 튼튼하고 간단하게 설치 가능 원단 : 박막 필름(물청소 가능) 케이스와 스크린 일체형으로 이동 용이 표면 구조 : Highter Power(Ultra Bright)

규    격    서

ITEM NO.	품명	수량
장-29	Audio System	2ea

규격	세부사양	비고
세부규격	출력 : 50W 스피커 : 8 인치 무선마이크(FWM-10A) 초슬림형 : 28(W)*160(H)*14(D) 초경량 : 72g (배터리포함) 휴대폰용 착탈식 목걸이 제공 사용전원 : AAA 1.5V * 3 (4.5V) 송신주파수 : 217.000~220.125 MHz 송신출력 : 10 mW 충전 AC220V (전기가 없는 곳에서도 사용 가능) 겸용 무선마이크, 유선마이크 및 외부입력 동시사용 신호출력단자 및 앰프출력단자 용도 : 50~100평 크기 : 280(W) * 330(H) * 210(D) 무게 : 8 Kg

규    격    서

ITEM NO.	품명	수량
장-30	Video Deck	2set

규격	세부사양	비고
세부규격	Recording/playback performance Recording format: 1080/60i, 1080/50i, 480/60i (NTSC), 576/50i (PAL) Playout/down conversion format: 1080/60i, 1080/50i, 480/60i (NTSC), 576/50i (PAL), 480/60P, 576/50P, 720/60P, 720/50P Tape speed: HDV/DV SP Max. 18.812 mm/s DVCAM Max. 28.218 mm/s Playback/recording time: HDV/DV SP Max. 276 min with PHDV-276DM cassette, Max. 63 min with PHDVM-63DM cassette, DVCAM Max. 184 min with PHDV-276DM cassette, Max. 41 min with PHDVM-63DM cassette Fast forward/rewind time: Approx. 2 min with PHDV-276DM cassette Input/output connectors/devices Video input/output: BNC x 2 Video signal: 1 Vp-p, 75 Ω unbalanced, sync negative S-video input/output: Mini-DIN 4-pin x 2 Y: 1 Vp-p, 75 Ω unbalanced, sync negative C: 0.286 Vp-p (NTSC), 0.3 Vp-p (PAL), 75 Ω unbalanced Component video output: BNC x 3, Y: 1 Vp-p (0.3 V, sync negative) Pr/Pb (Cr/Cb): 700 mVp-p (100% color bar), input impedance 75 Ωi.LINK: 4-pin HDMI output: 19-pin (type A), video: 1080/60i, 1080/50i, 480/60i (NTSC), 576/50i (PAL), 720/60P, 720/50P, 480/60P, 576/50P, audio: PCM 48 kHz/16-bit Phones: Stereo minijack (φ3.5 mm), 8 Ω loading LANC: Stereo mini-minijack (φ2.5 mm) Control S: Stereo minijack (φ3.5 mm) Audio input: RCA pin x 2 Input level: -10/-2/+4 dBu, input impedance: min. 47 kΩ unbalanced,max. input level: -10: +18 dBu (approx. 6 Vrms),-2: +24 dBu (approx. 12.5 Vrms), +4: +30 dBu (approx. 25 Vrms) Audio output: RCA pin x 2 Output level: -10 dBu (full bit -20 dB), impedance 47 kΩ, unbalanced in 60i mode, -10 dBu (full bit -18 dB), impedance 47 kΩ, unbalanced in 50i mode Impedance: max. 1 kΩ unbalanced LCD monitor: 2.7-inch type, approx. 211,200 dots (960 x 220), Clear Photo LCD Plus Mass: Approx. 4.3 kg (9 lb 8 oz) Power requirements: AC 120 V, 60 Hz Power consumption: 12 W (playback mode with LCD monitor on) Operating temperature: 5 to 40°C (41 to 104°K) Storage temperature: -20 to +60°C (-4 to 140°K) Supplied accessories: Remote commander (1), power cord (1), size AA batteries (2), cleaning cassette (1), operating instructions Carrying Hard Case 제작사양 포함.	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
장-31	V3	6ea

규격	세부사양	비고
세부규격	바이러스에서 스파이웨어까지 각종 악성코드에 대한 통합 보안 바이러스, 웜, 해킹은 물론 스파이웨어까지 인터넷을 통해 유입되는 각종 악성코드에 대해 검사, 치료, 차단하여 다양한 보안 위협으로부터 사용자의 시스템을 안전하게 보호 각종 비밀번호, 메일주소, 통장 또는 카드 번호 등 사용자의 주요한 개인 정보가 허가되지않은 외부자에 의해 유출 되는 것을 막는 기능으로써, 개인정보 유출 허가가 등록된 e-mail 주소, 특정 URL 외에 개인 정보 유출 시 이를 차단하고, Messenger를 통해 개인정보가 유출될 경우에도 차단 피싱 차단(Anti-phishing) 및 URL 필터링 사용자가 금융기관이나 특정 사이트 방문 시 피싱 사이트 여부를 확인하여 자동으로 접속을 차단하므로 피싱으로 인한 금전적인 피해를 미연에 방지 악성코드가 네트워크를 통해 사용자의 시스템에 침입한 경우, 치료와 동시에 감염자 IP를 추적하여 자동으로 차단하므로 사용자가 인지하지 못할 경우라도 보안위협에 대한 신속한 대처가 가능 네트워크로 유, 출입되는 사용자 시스템의 모든 트래픽 현황을 한눈에 볼 수 있어 웜 등 비정상적인 트래픽을 유발하는 악성코드의 접근 상태를 확인하여 신속하게 차단하므로 악성코드로부터 시스템을 보호 바이러스 메일 검사 및 스팸메일 차단(Anti-spam) 메일을 통해 유입되는 바이러스를 실시간으로 검사하여 감염된 메일을 차단 및 치료 쿠기, 임시 인터넷 파일, 열어본 페이지 목록 등 인터넷 사용 시 생성된 각종 파일을 깨끗하게 청소할 수 있으며, 메모리 최적화, 인터넷 최적화 기능을 통하여 항상 최적의 시스템 상태를 유지할 수 있으므로 보다 쾌적한 시스템 상태를 유지 파일 암호화 및 완전 삭제 사용자의 소중한 파일을 관리하기 위해 해당 파일을 암호화 하여 유출이 발생하더라도 안심 지정한 영역에 대한 빠른 검사, 일반 수동검사, 사용자 정의 검사 등 사용자 편의를 고려한 다양한 검사 방법을 제공 바이러스 검사 예약, 보안 취약점 진단 예약, 시스템 청소(Smart Cleaner) 예약, 시스템 최적화(Smart Optimizer) 예약 기능

운영 사무실

규    격    서

ITEM NO.	품명	수량
사-1	CCTV Camera	9ea

규격	세부사양	비고
세부규격	- 방송방식 EIA Standard : 525 Lines, 30Frames/sec - 촬상소자 : 1/3" IT CCD 27만 화소 - 유효화소수 : 510(H) × 492(V) - 주사방식 : 2:1 INTERLACE - 주사선 주파수 : 수평(INT/L.L) : 15.734KHz/15.750KHz - 수직(INT/L.L) : 59.94Hz/60Hz - 동기방식 : Internal/Line-Lock - 수평해상도 : 330본 이상 - 신호출력 : VBS 1.0Vp-p(75 ohm, composite) - S/N비 : 48dB 이하 - 최저조도 : 6.0Lux(40 IRE) - Shutter Speed : 1/60 ~ 1/100,000 - AGC : Auto - Lens f = 4.0mm(F2.0), C-Mount 착탈식 - 최대 Lens 가용 Size : (pi 30 x L28) - 입/출력단자 전원 : Phone Jack Type(센터 핀 +) - 영상 : BNC Type - 수평조정각도 : 0~355° - 수직조정각도 : 15°~ 90°(Lens에 따라 가변) - 입/출력 소켓 Video Output : BNC(rear) - AI Lens : 4-pin DIN(side) - Power : 2pin term.(rear) - Power Indicator : LED(rear) - 동작온도 : -10℃ ~ 50℃ - 동작습도 : 85%RH 이하 - 사용전원 : DC12V - 소비전력 : 2W

규    격    서

ITEM NO.	품명	수량
사-2	DVR	1ea

규격	세부사양	비고
세부규격	- 감시/녹화 속도 : XO 400 (16CH) : 480 fps / 240 fps (NTSC) - 비디오 방식 : NTSC / PAL 방식 자동 설치 - 압축 방식/압축률 : MPEG4 - 2~5 KB( 320 * 240 표준화질) - O/S : Win2000 - 해상도 : NTSC: 720*480, 320*240, PAL : 768*576, 384*288 - 비디오 In/Out : BNC 16Ch/3Ch (2 VGA Out, 1 TV Out) LoopThrough 출력지원(선택사항) - 오디오 In/Out : 2Ch(Line In) / 1Ch(Line Out) - 16Ch(선택사항) - 센서 In/Out : 16Ch (TTL)/16Ch (TTL) - 화면 분할 : 1,4,9,16,S6,S8 - 외부장치 : PTZ(RS-485, COM Port) - 센서 릴레이 : UPS등 지원 - 저장장치 : 기본 160GB - ( 400 GB 최대 4개 장착 가능: 1.6 TB) - 백업장치 : CD/DVD-RW, USB 2.0, Network 백업 - 네트워크 : LAN/ISDN/PSTN/ADSL etc - 본체치수 : 510 x 482 x 177 mm(19’’ rack mount type) - 본체중량 : 20.0 Kg - 동작온도 : 5~45 C - 동작습도 : 10% ~ 90% - 전원 : 100 ~ 250 VAC, 50/60 Hz

규    격    서

ITEM NO.	품명	수량
사-3	Monitor	1ea

규격	세부사양	비고
세부규격	- 화면 화면크기 : 32“ diagonal (800.4mm x 31.51mm) 화면비 : 16:9 해상도 : 1366(H) x 768(V) (WXGA) 픽셀 : 170.25㎛(H) x 510.75㎛(V) 표시색수 : 16.7 Billion Colors 시야각 : Over 170° 이상 명암비 : 1600:1 휘도 : 600cd/㎡ (Max) - 화질 입력신호 : 1080i / 720p / 480p / 480i 이중주사 : 이중주사 (Progressive Scan) 자동영상 : Cinema Progressive Scan - 후면연결단자 HDMI, Optical, Conponent, S-video, PC입력단자, 안테나 입력단자 AV 입력단자, PC오디오 아웃단자, A/S단자, 컨포넌트 아웃단자 - 제품무게 : 26kg, 28kg(포장) - 제품크기 : 985x489x110 (스텐드제외), 985x489x225(스텐드포함) - 전원 : AC 100V~240V, 50/60Hz - 소비전력 : 150W - 보관상태 : 온도 0°~40, 습도 20% ~ 80%

규    격    서

ITEM NO.	품명	수량
사-4	W/L internet System	1sys

규격	세부사양	비고
세부규격	- Standards IEEE 802.11a, 802.11b, 802.11g wireless LAN IEEE 802.3, 802.3u Ethernet IEEE 802.3x flow control IEEE 802.3af Power over Ethernet (PoE) IEEE 802.11h IEEE 802.11d - Data Transfer Rates For 802.11a/g: 108, 54, 48, 36, 24, 18, 12, 9 and 6Mbps For 802.11b: 11, 5.5, 2, and 1Mbps - Wireless Frequency Range** 2.4GHz to 2.4835GHz 5.15GHz to 5.35GHz and 5.47GHz to 5.85GHz - Radio and Modulation Type For 802.11b (DSSS): DBPSK @ 1Mbps DQPSK @ 2Mbps CCK @ 5.5 and 11Mbps For 802.11a/g (OFDM): BPSK @ 6 and 9Mbps QPSK @ 12 and 18Mbps 16QAM @ 24 and 36Mbps 64QAM @ 48, 54 and 108Mbps For 802.11a/g (DSSS): DBPSK @ 1Mbps DQPSK @ 2Mbps CCK @ 5.5 and 11Mbps - Typical T ransmit Output Power * FCC For 802.11a: 18dBm For 802.11b: 21dBm For 802.11g: 21dBm

규    격    서

ITEM NO.	품명	수량
사-4	W/L internet System	1sys

규격	세부사양	비고
세부규격	ETSI For 802.11a: 14dBm For 802.11b: 17dBm For 802.11g: 17dBm - Antenna Gain For 5GHz: 5.5dbi For 2.4GHz: 2.5dbi - Antennas Dual 5dBi Gain detachable diversity dipole antennas with reverse SMA connectors - Ethernet Interfaces LAN 1: 10/100BASE-TX port with 802.3af PoE LAN 2: 10/100BASE-TX port Two LAN ports can be simultaneously connected (with seperate SSID) - Operation Modes Access Point WDS with AP WDS/Bridge (no AP broadcasting) - Security 64-, 128-, 152-bit WEP data encryption MAC address filtering WPA/WPA2 EAP WPA/WPA2 PSK WPA PSK/AES over WDS AES 802.11i-ready 802.1Q SSID broadcast enable/disable Multiple SSIDs network segmentation 802.1Q security for each SSID (up to 208 VLAN groups/VLAN Tagging) Rogue AP detection

규    격    서

ITEM NO.	품명	수량
사-4	W/L internet System	1sys

규격	세부사양	비고
세부규격	- Device Management Web browser interface: HTTP Secure HTTP (HTTPS) AP Manager SNMP support: D-View module Private MIB Command Line Interface: Telnet Secure (SSH) Telnet - Diagnostic LEDs Power Status LAN 1 LAN 2 802.11b/g 802.11a - Certification FCC Class B CE C-Tick UL Wi-Fi - QoS : WMM (Wi-Fi multimedia certified) - Operating Voltage : 48VDC +/- 10% for PoE - Power Supply : Through 48DCV, 0.4A external power adapter - Power Consumption : 6.72 watts (140mA) (max.) - Dimensions 164.59 (L) x 184.66 (W) x 31.75 (H) (6.48 x 7.27 1.25 inches) - Weight : 603.28 grams (1.33 lbs)

규    격    서

ITEM NO.	품명	수량
사-5	DID system	1ea

규격	세부사양	비고
세부규격	1. 패널 : Lcd - 42" Network DID Vetical Display 42" Brightness : 450cd/m2~ Resolution : 1920 x 1080 Contrast Ratio : 1700:1 Viewing Angle : L/R:178, U/D:178 Settop PC 포함 Net workserver S/W including 2. 운영 소프트웨어 - 각종 멀티미디어 컨텐츠를 자유롭게 화면 편집하여 스케쥴링에 의하여 스트리밍 또는 다운로드 방식으로 원격지 디스플레이를 제어하는솔루션 - 템플릿에 의한 손쉬운 분할화면 선택 - 편리한 화면 크기 조정 - 스토리 보드 형태의 화면 편성 - 플래쉬, 동영상 이미지, TV, 웹 스트리밍 가능 - 실시간 예약 자막 가능화면분할, - 원격 진단 및 A/S 가능 - 다중 네트워킹 가능 - 터미널 정보 입력/수정/관리 - 월별, 주간별, 일별, 시간별, 반복 일정 입력기능 - 월간 일정, 당일 시간 별 일정 표기	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

상영관

규    격    서

ITEM NO.	품명	수량
상-1	4K Digital Projector	1set

규격	세부사양	비고
세부규격	디스플레이 장치 : SXRD (Silicon X-tal Reflective Display) 크기 : 1.55인치 (대각선) 해상도 : 4096 (가로)X2160 (세로) 픽셀 반사율 : 72% 명암 (소자 기준) : 4000:1 이상 픽셀 피치 : 8.5㎛ 간격 (픽셀 간) :0.35㎛ 응답 속도 : 5m/sec (tr+tf) 액정 모드 : 세로 정렬 모드 조정 층 : 무기질 박막 백플레인 공정 0.35㎛ MOS 공정 액정 셀 간격 2㎛ 프로젝션 시스템 : 3-SXRD 패널, 프리즘 컬러 통합 시스템 촬상 소자 : SXRD, 1.55인치 (대각선), 각 칩에 4096 (H)X2160 (V)픽셀 램프 : 2kW 제논 램프 (2) (SRX-R110) - 스크린 범위 : 14피트~51피트 (약 4.5m~15.5m) (가시 범위의 가로 길이) 밝기 : ● 10,000 ANSI 루멘 ±10% (SRX-R110/S110) 명암 : 1800:1 이상 해상도 : ● 600TV 라인 (SDI 입력/SMPTE-259M) ● 1920x1080 픽셀 (HD-SDI 입력, SMPTE-292M) ● 4096x2160 픽셀 (RGB) - Board & Accessories : ● SDI interface Board(LKRI-004) ● 2KW Xenon Lamp House ● HD-SDI Input Board (LKRI-002) ● Zoom Lens (LKRI-Z115)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-1	4K Digital Projector	1ea

규격	세부사양	비고
세부규격	신호 규격 : ● 비디오: 컴포넌트 (Y∙Cb∙Cr), HD (G∙B∙R/Y∙Pb∙Pr) ●컴퓨터: XGA, SXGA, UXGA ●DVI-D: XGA, Quad-VGA, SXGA, UXGA, WUXGA, 1920x1080, 2048x1080 사용 전원 : AC 200~240V, 50/60Hz 작동 온도 : +5℃~35℃ 보관 온도 : -20℃~+60℃ 작동 습도 : 35%~85% (비응결 시) 보관 습도 : 10%~90% 치수 (너비X높이X깊이) : 약 740x500x1,330mm 중량 : 약 110kg	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-2	Projector Rack	1ea

규격	세부사양	비고
세부규격	- 각도조절 : 30“ 이상 - 달리여부 : 4ea - 크기(WxHxD) : 600 x 900 x 450 mm - 무게 : 15 kg - 재질 : Steel - Rack여부 : 스탠다드 19“ 10U 이상

규    격    서

ITEM NO.	품명	수량
상-3	W/L Mic(Pin Type)	1ea

규격	세부사양	비고
세부규격	19" RACK MOUNTABLE UHF WIRELESS SYSTEM - Operating Frequency : RX-702DE : 740.250 ~ 751.750 ㎒ - Frequency Stability : ± 15 PPM - Receiver Sensitivity : 5 ㎶ - Audio Frequency Response : 60㎐ ~ 15㎑ (±3dB) - Signal to-Noise Ratio : More than 90dB - Maximum FM Deviation : 56K - Harmonic Distortion : 0.6% 이내 - Audio Frequency Output : - 40dBm ~ -25dBm (ADJ.) - Squelch : 0 ~ 30㎶ (ADJ.) - Pre-scaled channel : 10CH - Antenna Type : WHIP ANT - Power Supply : 220V/60㎐ ADAPTER - Dimension (W x H x D) : 483 x 44.5 x 214 (㎜) - Weight : 2.5kg BODY PACK TRANSMITTER - Operating Frequency : TX-755PM : 740.250 ~ 751.750 ㎒ - RF OUTPUT : 10㎽ - Audio Frequency Response (RX + TX) : 60㎐ ~ 15㎑ (±3dB) - Frequency Stability : ± 15 PPM - Signal to-Noise Ratio (RX + TX) : More than 90dB - Modulation : PLL Synthesizer - Harmonic Distortion (RX + TX) 1K : 0.6% 이내 - Pre-scaled channel : 5 / 10 / 16 / 48 Channels - Antenna Type : WHIP ANT - Operating Distance : 100m 이내 (장소에 따라 차이가 남) - Operating Time : 6 Hours - Power Supply : DC 3V (AA" 1.5 × 2) - Dimension (W x H x D) : 63 × 107 × 19 (㎜) - Weight : 110g (Without Batteries)

규    격    서

ITEM NO.	품명	수량
상-4	Wired mic.	4ea

규격	세부사양	비고
세부규격	- Frequency response : 60 Hz ~ 20 KHz - Sensitivity : -52.5 dB(0 dB = 1 V/Pa, 1KHz) - Impedance : 800 Ohm - Pick-up pattern : Super Cardioid - Power Supply : 1.5V Battary - Weight(g) : 154 - Color : Black, Silver

규    격    서

ITEM NO.	품명	수량
상-5	Mic Stand	4ea

규격	세부사양	비고
세부규격	- T-Type - Extendable boom Arm - Height : 95~170cm - Weight(g) : 3 kg

규    격    서

ITEM NO.	품명	수량
상-6	Blue-ray Player	1ea

규격	세부사양	비고
세부규격	- 재생디스크 : MP3/BD/DVD/CD/JPEG/HD JPEG - 비디오 : ●비디오압축포맷:VC-1,MPEG2,H.264,HD JPEG ●비디오DAC:10bit/108Mhz ●출력해상도:1920 x 1080 P/1920 x 1080 I /1280 x 720 P/720 x 480 P /720 x 480 I - 비디오스테일링:DVD 스케일링 - 오디오 : ●오디오압축포맷:Dolby Digital,DTS,DTS HD High Resolution Audio,Dolby TrueHD,Dolby Digital plus,MP3 ●오디오DAC:24bit/192Khz - 영상 출력 : S-비디오 HDMi - 디지털 오디오 출력 : OK - 소비전력 : 29W - 전원 : AC 220V 60Hz - 사이즈(W*D*H) : 430x79x325 - 무게 : 4.2kg with - Component---DVI Converting Gender

규    격    서

ITEM NO.	품명	수량
상-7	HDV Player	1ea

규격	세부사양	비고
세부규격	- Recording format HDV: HDV1080/60i, 1080/50i, 1080/24p, 1080/25p, 1080/30p DVCAM/DV SP: DVCAM,DV SP 480/60i (NTSC), 576/50i (PAL) - Playout format HDV: HDV1080/60i, 1080/50i, 1080/24p, 1080/25p, 1080/30p. HDV720/24p, 720/25p, 720/30p DVCAM/DV SP:DVCAM,DV SP 480/60i (NTSC), 576/50i (PAL) - Playout video signal 1080/60i, 1080/50i, 480/60i (NTSC), 576/50i (PAL), 480/60P, 576/50P, 720/60P, 720/50P - Tape speed HDV/DV SP: Max. 18.812 mm/s DVCAM: Max. 28.218 mm/s - Playback/recording time- HDV/DV SP: Max. 276 min with PHDV-276DM cassette Max. 63 min with PHDVM-63DM cassette DVCAM: Max. 184 min with PHDV-276DM cassette Max. 41 min with PHDVM-63DM cassette - Fast forward/rewind time : Approx. 2 min with PHDV-276DM - Video input/output : BNCx1 / BNCx1 - Monitor video out : RCA pin x1 - S-video input/output : Mini-DIN 4-pin x1 / Mini-DIN 4-pin x1 - Component video output : BNC x 3 - i.LINK interface (HDV /DV) : 6-pin (no power) - HD/SD-SDI output : BNC x1 - Audio input : RCA pin x 4ch - Audio output : XLR 3pin x 4ch - Monitor audio out : RCA pin x 1 - AES/EBU output : BNC x2 - TC out : BNC x1	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-7	HDV Player	1ea

규격	세부사양	비고
세부규격	- Phones : Stereo minijack (ø3.5 mm) - LANC : Stereo mini-minijack (ø2.5 mm) - Control S input : Stereo minijack (ø3.5 mm) - LCD monitor : 2.7-inch type (Viewable area measured diagonally), approx. 211,200 dots (960 x 220), Clear Photo™ LCD Plus - Weight : Approx. 9 lb 12 oz (4.4 kg) Dimensions (WxHxD): Approx. 212 x 88 x 390.3mm (8 3/8 x 3 1/2 x 15 3/8 inch) Power requirements : AC 120 V, 60 Hz Power consumption : 16 W (playback mode with LCD monitor on) Operating temperature : 41 to 104 °F (5 to 40 °C) Storage temperature : -4 to 140 °F (-20 to +60 °C)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-8	HDD Player	1set

규격	세부사양	비고
세부규격	- 메인칩셋 : 시그마 디자인 EM8621 - VFD 디스플레이 : 재생모드, 재생시간, 해상도 (문자 7자, 숫자 5자) - 비디오포맷 : avi, wmv, mpg, iso, vob, ifo, mp4, asf, tp, trp, ts - 비디오코덱 : MPEG 1/2/4, AVI, XVID, WMV9 - 해상도 : 최대 1920 x 1080i - 오디오포맷 : MP3, WMV, AAC, Ogg, PCM, AC3, M4A, FLAC, WAV DTS 다운믹싱과 패스 스루 - 이미지 : JPEG 지원 - 연결 확장 : USB 2.0 Host 2 포트, USB 2.0 타겟 1 포트 LAN (10/100Mbps) 지원 - 비디오 출력 : 비디오 DVI, 콤포넌트, S- Video, Composite - 오디오 출력 : 디지털 - 코엑시얼, 광출력. 아날로그 - 스테레오 - 지원 HDD : SATA HDD (NTFS, FAT 32) DTV 녹화 : NTFS 포맷 7200 rpm HDD - ODD 지원 : USB 2.0 호스트로 연결 사용 가능 - 자막 지원 : smi, sub, sub/idx, Irc, txt, srt - 쿨링팬 : 속도 조절 가능 (자동 온도 감지 속도 조절) - 메인 메모리 : 64M byte - 플래시 메모리 : 8M byte - 파워 : 내장 프리볼트 제품 - 지원 언어 : 한글, 영어, 일어, 불어, 독어, 스페인어, 이태리어, 포루투칼어, 스웨덴어, 노르웨이어, 중국어 - 크기 : 183 x 139 x 75 mm - 무게 : 1,300g (하드디스크 포함)

규    격    서

ITEM NO.	품명	수량
상-9	LCD Viewing Monitor	1ea

규격	세부사양	비고
세부규격	- 화면 크기 : 43 cm/17 inch - 표시화면크기 (HxV) : 337.92x270.34 mm(HxV) - Pixel Pitch (HxV) : 0.264 x 0.264 mm - 해상도 : 1280x1024 - 표면코팅처리 : Anti-Glare Hard Coating(3H) - 표시색상 : 16.2 M Colors - 밝기 : 300 cd/㎡ - 응답속도 : 5 ms - Contras비 : 2000:1 - 시야각 : 170도 - 수평주파수(Digital) : 30~83 kHz - 수직주파수(Digital) : 56~75 Hz - 신호입력 : Analog / Digital - 입력 해상도 : 1280x1024 - Interface : D-Sub / DVI-D - Power Supply : 90 ~ 264 Vac - 소비전력 : 30W(On), 1W(stand by, Off) - 크기(WxHxD) : 365 x 378 x 180 mm - 무게 : 3.1 kg

규    격    서

ITEM NO.	품명	수량
상-10	Audio Monitor	1pair

규격	세부사양	비고
세부규격	General Type: Biamp. 2-way, bass-reflex powered speaker General Crossover Frequency: 2.5kHz General Overall Frequency Response: 50 Hz ~ 40kHz Dimensions (W X H X D): 169mm x 279mm x 222mm (6 5/8 in. x 11 in. x 8 in.) Weight: 7.5kg (16.5 lbs) Speaker Components: LF: 12cm (4 2/7 in.) cone (4 ohms) HF: 2.5cm (1 in.) titanium dome (6 ohms) Speaker Enclosure: Bass reflex type, magnetic shielding construction Amplifier Output Power: LF: 40W at 400Hz, THD=0.02%, RL=4 ohms HF: 27W at 10kHz, THD=0.02%, RL= 6 ohms Amplifier Input Sensitivity/ Impedance: Line 1: +4dB/10k ohm/XLR Line: 2 -10dB/10k ohm/Phone Jack Amplifier S/N: Greater than or equal to 100dB (A weighted) Amplifier Controls: TRIM switches: LOW: 4 position (+1.5dB, 0dB, -1.5dB, -3.0dB at 60Hz); HIGH: 3 position (+1.5dB, 0dB, -1.5dB, at 15kHz); Power switch: On/Off; Level Control Amplifier Power Indicator: Green LED Amplifier Power Requirement: 120v 60Hz Amplifier Power Consumption: 60W

규    격    서

ITEM NO.	품명	수량
상-11	Headphone	1ea

규격	세부사양	비고
세부규격	- Connector Type: 1/8 - Weight: 9.9 - Isolation: -15dB - Detachable Cable: No - Impedance @ 1kHz: 64 - Coupler Size: Large - Cord Type: Coiled Left-Side - Cord Length: 10 ft. - Ear Coupler Type: Full-Size - Driver Type: Dynamic - Acoustic Seal: Sealed - Headphone Type: Head Set

규    격    서

ITEM NO.	품명	수량
상-12	Audio Mixer	1ea

규격	세부사양	비고
세부규격	- Channels: 16 mono + 4 stereo - Mono Mic/Line Channel Inputs: 16 ("Invisible" Mic Preamps +1/4 TRS balanced) - Stereo Line Channel inputs: 8 - Channel Inserts: 16 - EQ Mono Channels: 3-band mid-sweep + low cut - EQ Stereo Channels: 4-band - Phantom Power: +48V - Aux Sends: 2 (pre/post fader switchable) - FX sends: 2 (post fader) - Stereo FX Returns: 2 - Subgroups: 4 - Main Mix Outputs: 2 (with XLR & 1/4" TRS connectors each) - Main Mix Inserts - Mono Subwoofer Output: Adjustable from 30-200 Hz - 2-track I/O RCA Connectors - Phones/Control Room Output - PFL/Solo Section - FX Units with Footswitch Connector: 2 (24-bit/99 presets each) - Stereo Graphic EQ: 9-band - FBQ Feedback Detection System - Talkback Section with Internal Mic - Standby Switch (mutes all channels) - Auto-Range Power Supply: 100-240 V - Height x Width x Depth (approx.): 100 x 682 x 410 mm; 3.94 x 26.87 x 16.15" - Weight (approx.): 8.5kg; 18.7 lbs.

규    격    서

ITEM NO.	품명	수량
상-13	Surround 7.1Ch Amp	1set

규격	세부사양	비고
세부규격	- Channels : 7 - RMS Output Power : (20Hz - 20kHz) 140W x 7 - Total Power : (20Hz - 20kHz) 980W - Dolby Digital EX/ Dolby Pro Logic IIx - DTS-ES Discrete 6.1, DTS 96/24 / DTS Neo:6 - iPod Compatibility - Compressed Music Enhancer - Neural Surround - XM HD Surround - XM Satellite Radio Ready - HDMI (In/Out) (3 / 1) V1.2a - Component Video (In/Out) (3 / 1) - A/V Inputs (S-Video) 6 (All S-Video) - Digital Inputs/Outputs [O: Optical, C: Coaxial] (O: 5, C: 3 / O: 2) - Front A/V with Digital Input : (S-Video / Optical) - Time Base Corrector - HDMI Up Conversion : (Scale to 480p/ 720p/ 1080i) - Component Video Up Conversion - S-Video Up Conversion - Dialogue Lift - YPAO (w/Optimizer Microphone) - On-Screen Display : (With GUI) - Assignable Power Amp - Zone Speaker Terminals : (Zone 2 / 3) - Zone 2 Output :(With Composite video) - Zone 3 Output :(Audio Only) - Selectable Subwoofer Crossover - Multi-Channel Decoder Inputs 8-Channel - Pre-Out All Channels - Learning Remote Capability - Macro Command Capability - Product Dimensions (W x H x D) :17-1/8" x 6-3/4" x 17-1/4" - Product Weight (lbs.) :37.9 - Shipping Dimensions (W X H X D) :20-3/4" x 10-3/4" x 21" - Shipping Weight (LBS) :44

규    격    서

ITEM NO.	품명	수량
상-14	3-way main stage speaker	3ea

규격	세부사양	비고
세부규격	-Frequency Range: 30 Hz to 20 kHz (-10 dB) - Frequency Response: 45 Hz to 12 kHz (+/- 3 dB) - Power Capacity: 300 Watts Passive HF: 50 Watts Bi-Amp LF: 600 Watts Bi-Amp - Sensitivity: 98 dB (1W, 1m) - Nominal Impedance: 8 Ohms - Crossover Frequency: 1 kHz - Nominal Coverage: 90° Horizontal, 90°Vertical - Half-Space Reference Efficiency: 3.3% - Maximum Acoustic Power Output: 8 Acoustic Watts (Sine Wave Input) - System Polarity: Positive Voltage to RED produces forward cone motion - Input Connectors: Barrier Strip Screw Terminals - Dimensions (HxWxD): 1019 (w/horn) x 651 x 292 mm (40.125 (w/horn) x 25.625 x 11.5 in) - Net Weight: 41 kg (90 lbs)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-15	Subwoofer speaker	1ea

규격	세부사양	비고
세부규격	- Frequency range (–10 dB): 28 Hz to 500 Hz - Frequency response (± 3 dB): 38 Hz to 100 Hz - Power capacity : 300 W - Sensitivity: 100 dB (1W, 1m) - Nominal impedance: 8 ohms - Recommended crossover frequency: 100 Hz - Half-space reference efﬁciency: 5% - Maximum acoustic power output (sine wave input) : 15 W IEC standard - System Polarity: Positive voltage to RED produces forward cone motion - Input connectors: Barrier strip screw terminals - Net system weight: 51 kg (113 lbs) - Shipping weight: 54 kg (119 lbs) - Dimensions (H x W x D): 1168 x 651 x 368 mm ( 46 x 25.625 x 14.5 inches)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-16	Surround speaker	6ea

규격	세부사양	비고
세부규격	- Frequency Range: 40 Hz to 20 kHz (-10 dB) - Frequency Response: 100 Hz to 12 kHz (+/- 3 dB) - Power Capacity (Continuous Pink Noise): 75 Watts - Sensitivity: 89 dB (1W, 1m) - Nominal Impedance: 8 Ohms - Crossover Frequency: 2.5 kHz - Nominal Coverage: 100° Horizontal, 100°Vertical - System Polarity: Positive Voltage to RED produces forward cone motion - Input Connectors: Barrier Strip Screw Terminals - Dimensions (HxWxD): 446 x 483 x 267 mm (17.5 x 19 x 10.5 in) - Net Weight: 13 kg (29 lbs)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-17	Surround bracket	6ea

규격	세부사양	비고
세부규격	- Material: Alloy steel - Finish: Powder coat paint - Color: Black - Working Load: 20 lbs. (9 kg) - Design factor: 10:1 ratio - Net Wgt: 1.5 lb. (.7 kg) each - Shipping wgt:4 lbs. (1.8 kg) pair - Pack count:2 units/carton	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-18	Power Amp.	5ea

규격	세부사양	비고
세부규격	20 Hz-20 kHz:10 dB below rated power : Less than 0.01% THD, 4 & 8 1.0 kHz below:full rated power : Less than 0.01% THD, 4 & 8 Frequency Response : 20 Hz-20 kHz,± 0.2 dB / 8 Hz-50 kHz, +0, -3 dB Damping Factor (1 kHz and below): Greater than 500 Input Impedance : 10 K unbalanced, 20 K balanced Input Clipping : 10 Vrms (+22 dBu) Cooling : Variable-speed fan, rear-to-front air flow Connectors (each channel) : Input: 1/4" TRS, 3-pin XLR and 3-pin detachable terminal blocks (1 each per channel) Output: Neutrik Speakon™ and safety-shrouded barrier strip, including monitor output Controls Front: AC switch, Ch.1 and Ch.2 gain knobs Rear:DIP switch for Ch.1 and Ch.2:clip limiter on/off,LF filter on/off,LF filter freq select-30 or 50 Hz; inputs parallel or stereo; bridge mode Indicators: PARALLEL INPUTS: Yellow LED CLIP/PROT: Red LED BRIDGED: Yellow LED LEVEL -10 dB: Green LED PWR-ON: Green LED LEVEL -20 dB: Green LED SIGNAL -35dB: Green LED (1 per channel) Amplifier Protection : Full short circuit,open circuit,thermal,ultrasonic,and RF protection.Stable into reactive or mismatched loads Load Protection : On/off muting, DC-fault power supply shutdown Dimensions : 19" (48.3 cm) rack mounting, 3.5" (8.9 cm) tall (2 rack spaces), 14" (35.6 cm) deep (from front mounting rails) Voltage Gain 40x (32 dB) Weight :21 lb (9.5 kg) net Optional Accessories: The XC-3 Cinema Crossover is for bi-amp applications The SF-3 Subwoofer Filter is an adjustable highpass filter The LF-3 Low Frequency Filter is used with the XC-3 The DSP-3 digital signal processor features crossover filters plus numerous The DSP-4 digital signal processor provides all features of the DSP-3,but with a higher signal to noise ratio.(XLR connectors)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
상-19	Micro Hall Screen	1ea

규격	세부사양	비고
세부규격	- By user format after fixing the diagram for theater - Pearl Lux Hole Screen 8*5 - Gain ● Front : 2.5±10% ● Side : 0.7±10% - 마스킹 - 스크린 사이즈 : 인테리어가 허용하는 최대 사이즈 구현 - 펄 코팅 - 방염 처리 - 프레임 배플 형 - 마이크로 홀 스크린

규    격    서

ITEM NO.	품명	수량
상-20	Screen Protector	1ea

규격	세부사양	비고
세부규격	- Velvet 12*9 - Soft material made from cotton, silk, or nylon - 설치 스크린을 보호하는기능

규    격    서

ITEM NO.	품명	수량
상-21	AL Rack	1ea

규격	세부사양	비고
세부규격	- 재질 : STEEL 2.0T, 1.6T, 1.2T 19” Rack Mount - Aluminum Frame - W : 570 - W" : 483 - D : 650, 750, 900 - D" : 503, 603, 753 - H : 858 - H" : 668

규    격    서

ITEM NO.	품명	수량
상-22	I Type office Desk	1ea

규격	세부사양	비고
세부규격	- 책상 크기 : 1600*1200*750 - 책상 : 우드 월 넷, “L” 형 - 의자 : 편안하고 인체공학적인 사무용 의자 * 색상 및 세부 규격은 협의 후 결정

규    격    서

ITEM NO.	품명	수량
상-23	Installation& Materials	1lot

규격	세부사양	비고
세부규격	Equipment Setting Cable Connecting Cable Wiring Warraty Service Hiding Cable Fixing Equipment H/W Testing Desk & Chair Setting * including Mike Wall box (2ea)

아카이브실

규    격    서

ITEM NO.	품명	수량
아-1	LCD Display	4ea

규격	세부사양	비고
세부규격	- 제품 분류 : 24 인치 - 화면 비율 : 16:10 - 최대 해상도 : 1920 x 1200 - 명암비 : 700 : 1 - 밝기(㎡) : 400 cd - 응답 속도(ms) : 6 ms - D-SUB : 1개 - DVI : 1개 - 컴포지트 : 1개 - S-VHS : 1개 - 컴포넌트 : 1개 - TV 수신 : 지원 - 내장 스피커 : 지원

규    격    서

ITEM NO.	품명	수량
아-2	DVD/VHS Player	4ea

규격	세부사양	비고
세부규격	Product Type DVD recorder/ VCR combo Width 43 cm Depth 26 cm Height 7.9 cm Features Progressive scanning (line doubling) Output Mode Stereo Digital Audio Format Dolby Digital output, DTS digital output Surround Sound Effects 3D Surround Optical Digital Output Yes Coaxial Digital Output Yes Type DVD recorder Media Type CD-R, CD-RW, DVD-R, DVD+RW, DVD-RW, DVD+R, DVD, CD, Video CD, DVD+R DL Recordable Media DVD-R, DVD-RW, DVD+RW, DVD+R Recording Mode XP, SP, LP, EP, MLP Supported Digital Video Standards DivX, XviD Supported Digital Audio Standards WMA, MP3 Picture Zoom Yes MP3 Compatible Yes DVD Additional Features JPEG photo playback, ID3 tags support Device Type VCR Media Type VHS TV Tuner Tuner Qty 1 Reception System PAL, SECAM Connector Type 1 x RF input ¦ 1 x RF output ¦ 1 x IEEE 1394 (FireWire/i.LINK) ¦ Audio line-out ( RCA phono x 2 ) ¦ 1 x SPDIF output ( RCA phono ) ¦ 1 x SPDIF output ( TOS Link ) ¦ 1 x S-Video output ( 4 PIN mini-DIN ) ¦ 1 x component video output ( RCA phono x 3 ) ¦ 2 x SCART ( 21 PIN SCART )

규    격    서

ITEM NO.	품명	수량
아-3	Headphone	6ea

규격	세부사양	비고
세부규격	Closed, dynamic, supra-aural headphones High efficiency drivers Wind-up belt clip for excess cable 10 foot Y style cable Replaceable leatherette ear pads Jack plug: 3.5/6.3 mm stereo Nominal impedance: 32 Ohm Weight w/o cable: ca. 130 g Transducer principle: Dynamic, closed Ear coupling: Supraaural Cable length: 3 m Frequency response (headphones): 18-18000 Hz Sound pressure level (SPL): 115 dB(SPL) THD, total harmonic distortion: Less than 0.5 percent

규    격    서

ITEM NO.	품명	수량
아-4	Headphone Distributor	2ea

규격	세부사양	비고
세부규격	- Provides maximum conductivity - Prevents corrosion - 24k gold-plated connectors and contacts - 2 stereo headphones or speakers to the mini-stereo jack

규    격    서

ITEM NO.	품명	수량
아-5	Library Desk	4ea

규격	세부사양	비고
세부규격	- 영상 감상용 책상으로 철재 및 목재를 사용하여 견고하고 미려하게 제작 - 색상 및 디자인은 공간 구성과 조화 되도록 협의 후 제작 - Dimension(L) x (D) x (H) : 1100 x 750 x 700

규    격    서

ITEM NO.	품명	수량
아-6	Chair 1	2ea

규격	세부사양	비고
세부규격	- 안락하고 편안한 구조로 PC사용자에게 편안한 사용이 가능. - LCD 비디오 감상용 테이블과 인테리어적으로 조화 - 크롬 도금 및 스테인레스 재질로 튼튼하고 안전한 구조 - 장시간 앉아 있어도 편안한 설계. - 심플한 디자인의 팔걸이는 발포 우레탄 소재 사용 - 스틸파이프에 의한 탄력 제공 - 팔걸이유 - 크기 : 575×610×890 - 몸체재질 : POLY PROPYLENE

규    격    서

ITEM NO.	품명	수량
아-7	Chair 2	2ea

규격	세부사양	비고
세부규격	- 안락하고 편안한 구조로 PC사용자에게 편안한 사용이 가능. - LCD 비디오 감상용 테이블과 인테리어적으로 조화 - 크롬 도금 및 스테인레스 재질로 튼튼하고 안전한 구조 - 장시간 앉아 있어도 편안한 설계. - 심플한 디자인의 팔걸이는 발포 우레탄 소재 사용 - 스틸파이프에 의한 탄력 제공 - 팔걸이유 - 2인용 - 크기 : 1300×610×890 - 몸체재질 : POLY PROPYLENE

다목적 강의실

규    격    서

ITEM NO.	품명	수량
다-1	Projector	1ea

규격	세부사양	비고
세부규격	Brightness - ANSI Lumens : 4,000 Contrast Ratio - Full ON/OFF : 500:1 Illumination Uniformity : 85% Imaging System : 0.8" Polysilicon TFT active matrix Panel x 3 Imaging System : Auto: H Sync. 15-100 kHz ~ V Sync. 50-100 Hz Screen Pixels : 1024 x 768 in stripe configuration Lamp : 300W lamp Estimated Lamp Life Hours : 2000 Computer Native Resolution : 1024 x 768 Computer Compatiblity: UXGA (Compression) / WXGA(Compression) / SXGA (Compression) / XGA / SVGA / VGA Computer Formats Supported : 1600x1200 through 640x480 Computer Dot Clock : 140 MHz Computer Image Sizing : Normal or Smart compressed or expanded Amplifier : Monaural 1W rms (T.H.D 10%) Speakers (Built-in) : 2.8cm 1pce Dimensions : 334(W) x 78(H) x 232(D) mm Net weight : 3.3 kg Packaged dimensions : 420(W) x 214(H) x 365(D) mm Packaged weight : 5.4 kg Operating Temperature - Max. : 95F (35C) Operating Temperature - Min. : 41F (5C) Generated Heat : 1314 BTU (331 KC)	입찰시 제조자 증명원 및 A/S 기술 지원확약서 필수첨부

규    격    서

ITEM NO.	품명	수량
다-2	Elec. Screen	1ea

규격	세부사양	비고
세부규격	- 스크린 재질 : 매트 화이트 - 반사 계수 : 정면: 0.8± 10% / 측면 : 0.8± 10% - 계폐 방식 : 전동식 - 크기 : 240 X 180Cm (가로X세로)

규    격    서

ITEM NO.	품명	수량
다-3	DVD/VHS Player	1ea

규격	세부사양	비고
세부규격	Product Type DVD recorder/ VCR combo Width 43 cm Depth 26 cm Height 7.9 cm Features Progressive scanning (line doubling) Output Mode Stereo Digital Audio Format Dolby Digital output, DTS digital output Surround Sound Effects 3D Surround Optical Digital Output Yes Coaxial Digital Output Yes Type DVD recorder Media Type CD-R, CD-RW, DVD-R, DVD+RW, DVD-RW, DVD+R, DVD, CD, Video CD, DVD+R DL Recordable Media DVD-R, DVD-RW, DVD+RW, DVD+R Recording Mode XP, SP, LP, EP, MLP Supported Digital Video Standards DivX, XviD Supported Digital Audio Standards WMA, MP3 Picture Zoom Yes MP3 Compatible Yes DVD Additional Features JPEG photo playback, ID3 tags support Device Type VCR Media Type VHS TV Tuner Tuner Qty 1 Reception System PAL, SECAM Connector Type 1 x RF input ¦ 1 x RF output ¦ 1 x IEEE 1394 (FireWire/i.LINK) ¦ Audio line-out ( RCA phono x 2 ) ¦ 1 x SPDIF output ( RCA phono ) ¦ 1 x SPDIF output ( TOS Link ) ¦ 1 x S-Video output ( 4 PIN mini-DIN ) ¦ 1 x component video output ( RCA phono x 3 ) ¦ 2 x SCART ( 21 PIN SCART )

규    격    서

ITEM NO.	품명	수량
다-4	5.1 ch Speaker	1ea

규격	세부사양	비고
세부규격	1. Woofer : Out-put Power : 70W RMS Woofer Drive : 6 1/2 Power in-put : 220V 60Hz Frequency Respones : 45Hz-180Hz Nominal Impedance : 4Ω In-put Sensitivity : 340mV S/N Ratio : 90dB Dimensions : 349(W) x 256(H) x 435(D) mm 2. Front Speaker : Midrange : 3 1/2", Tweeter : 1" Power Hendling : 20W~60W RMS x 2 Instant Power : 60RMS x 2 Sensitivity : 86db, Nominal Impedance : 4Ω Frequency Range : 180Hz ~ 20KHz In-put Sensitivity : 340mV Dimensions : 148(W) x 1089(H) x 145(D) mm 3. Center Speaker : Midrange : 3 1/2", Tweeter : 1" Power Hendling : 15W~45W RMS Instant Power : 45W RMS Sensitivity : 85db, Nominal Impedance : 4Ω Frequency Range : 180Hz ~ 20KHz Dimensions : 400(W) x 148(H) x 140(D) mm 4. Surround Speaker : Midrange : 3 1/2" Tweeter : 1" Power Hendling : 15W~45W RMS Instant Power : 45W RMS Sensitivity : 85db, Nominal Impedance : 4Ω Frequency Range : 180Hz ~ 20KHz Dimensions : 148(W) x 1089(H) x 145(D) mm

규    격    서

ITEM NO.	품명	수량
다-5	W/L Mic w/ Pin&Handheld	1set

규격	세부사양	비고
세부규격	19" RACK MOUNTABLE UHF WIRELESS SYSTEM - Operating Frequency : RX-702DE : 740.250 ~ 751.750 ㎒ - Frequency Stability : ± 15 PPM - Receiver Sensitivity : 5 ㎶ - Audio Frequency Response : 60㎐ ~ 15㎑ (±3dB) - Signal to-Noise Ratio : More than 90dB - Maximum FM Deviation : 56K - Harmonic Distortion : 0.6% 이내 - Audio Frequency Output : - 40dBm ~ -25dBm (ADJ.) - Squelch : 0 ~ 30㎶ (ADJ.) - Pre-scaled channel : 10CH - Antenna Type : WHIP ANT - Power Supply : 220V/60㎐ ADAPTER - Dimension (W x H x D) : 483 x 44.5 x 214 (㎜) - Weight : 2.5kg BODY PACK TRANSMITTER - Operating Frequency : TX-755PM : 740.250 ~ 751.750 ㎒ - RF OUTPUT : 10㎽ - Audio Frequency Response (RX + TX) : 60㎐ ~ 15㎑ (±3dB) - Frequency Stability : ± 15 PPM - Signal to-Noise Ratio (RX + TX) : More than 90dB - Modulation : PLL Synthesizer - Harmonic Distortion (RX + TX) 1K : 0.6% 이내 - Pre-scaled channel : 5 / 10 / 16 / 48 Channels - Antenna Type : WHIP ANT - Operating Distance : 100m 이내 (장소에 따라 차이가 남) - Operating Time : 6 Hours - Power Supply : DC 3V (AA" 1.5 × 2) - Dimension (W x H x D) : 63 × 107 × 19 (㎜) - Weight : 110g (Without Batteries)

규    격    서

ITEM NO.	품명	수량
다-5	W/L Mic w/ Pin&Handheld	1set

규격	세부사양	비고
세부규격	UHF BAND HANDHELD TRANSMITTER - Operating Frequency : TX-758M : 740.250 ~ 751.750 ㎒ - RF OUTPUT : 10㎽ - Audio Frequency Response (RX + TX) : 60㎐ ~ 15㎑ (±3dB) - Frequency Stability : ± 15 PPM - Signal to-Noise Ratio (RX + TX) : More than 90dB - Modulation : PLL Synthesizer - Harmonic Distortion (RX + TX) 1K : 0.6% 이내 - Pre-scaled channel : 10 Channels or 16 Channels - Antenna Type : WHIP ANT - Operating Distance : 100m 이내 (장소에 따라 차이가 남) - Operating Time : 6 Hours - Power Supply : DC 3V (AA" 1.5 × 2) - Dimension (W x H x D) : 51 × 239 × 51 (㎜) - Weight : 10CH : 220g (Without Batteries)

규    격    서

ITEM NO.	품명	수량
다-6	AV Processor	1set

규격	세부사양	비고
세부규격	Rated output *THD figures are power amp stage values Front : 75 W + 75 W (8 ohms, 20Hz - 20kHz) Centre : 75 W (8 ohms, 20Hz - 20kHz) Surround : 75 W + 75 W (8 ohms, 20Hz - 20kHz) Surround back : 75 W + 75 W (8 ohms, 20Hz - 20kHz) IN-put : HDMI, Component, S-Video, Composite, Analog audio, Digital OPT, Digital COAX, iPod ready Out-put : HDMI, Component, S-Video, Composite, Analog audio, Pre out 0.1ch Input sensitivity/impedance : Audio inputs - 200 mV/47 kohms Output level/Load impedance : Rec. Audio outputs - 200 mV/47 kohms Power supply : AC 230 V, 50 Hz Dimensions (WxHxD) : 434 x 171 x 383 mm Weight : 10.9 kg

규    격    서

ITEM NO.	품명	수량
다-7	Mixer	1ea

규격	세부사양	비고
세부규격	Total # Of Inputs : 14 - Balanced 1/4" TRS Phone Inputs Mic/Line Inputs : 6 - Balanced XLR Mic Inputs Stereo Line Inputs : 4 - Stereo Paired Balanced 1/4" TRS Phone (Channels 7-14) AUX Sends : 2 - 1/4" TRS Phone with extra 15dB of gain above Unity AUX Returns : 2 Stereo (4 mono) - 1/4" TRS Phone Inserts : 4 - 1/4" TRS Phone Pre-Fader/Pre EQ BUS (Group) Outputs : 4 - Group Outputs via ALT 3-4 output and Master Main Outputs 2 Trk Master I/O : Main Output L/R - Balanced 1/4" TRS Phone, L/R - Balanced XLR male switchable bettween mic and +4dB line level ALT I/O : Tape Input/Output L/R RCA-pin Monitor Outputs : Control Room L/R Balanced 1/4" TRS Phone Phones Single 1/4" TRS Phone HI Shelving +/- 15dB @12kHz MID Peaking +/- 12dB @2.5kHz LOW Shelving +/- 15dB @80Hz Solo/Mute : MUTE/ALT 3-4 switches on channels 1-12 SOLO (pre/post fader switchable) on channels 1-12 Channel Level Control : 60mm long-wearing log-taper faders Trim/Gain Control : Unity to +60dB Phantom Power : +48V Metering : 12 - segment peak LED's with "RUDE SOLO" light Frequency Response : 20Hz to 60kHz: +0 dB/-1 dB 20Hz to 100kHz: +0 dB/-3 dB Dynamic Range : 130dB Dynamic Range Signal-to-Noise Ratio : -100dBu; Main Mix knob down, channel Gain knobs down Total Harmonic Distortion (THD) : (1kHz @ 35dB gain, 20Hz-20 kHz bandwidth) Mic pre @ insert: 0.0007% Power Supply : 120VAC, 50/60Hz, 25 watts Weight : 9.5 lbs (4.5 kg)

규    격    서

ITEM NO.	품명	수량
다-8	A/V Rack	1ea

규격	세부사양	비고
세부규격	홈시어터, DVD, VDP 기기용 이동바퀴 : 블랙, 월넛 제품크기 : 가로 600 x 높이 860 x 깊이 420 상판유리 : 10T 평유리 선반유리 : 8T 평유리 2장 (높낮이조절 가능) 재질, 마감 : Chamber / 평유리 / 크롬장식 / DIY

규    격    서

ITEM NO.	품명	수량
다-9	Education Foldable Desk	10ea

규격	세부사양	비고
세부규격	- 가스 실린더를 사용한 원터치 폴딩시스템으로 부드러운 조작 - 스토퍼가 달린 캐스터를 사용하여 이동 용이 - 4면 우레탄 엣지로 제작 마감하여 미려하고 내구성이 강함 - 사용하지 않을 경우 접어서 보관하는 방식으로 공간 효율성극대화 - 규격 : 1800 x 450 x 740 - 기타 부품 포함. - 색상은 협의후 지정

규    격    서

ITEM NO.	품명	수량
다-10	Education Foldable Chair	30ea

규격	세부사양	비고
세부규격	- 심플한 디자인의 팔걸이는 발포 우레탄으로 제작되어 안락 - 스틸 파이프에 의한 탄력 제공 - 안락하고 편안한 구조로 사용자에게 편안한 사용이 가능. - 크롬 도금 및 스테인레스 재질로 튼튼하고 안전한 구조 - 장시간 앉아 있어도 편안한 설계. - 중간 등받이 - 스틸파이프에 의한 탄력 제공 - 팔걸이유 - 크기 : 575×610×890 - 몸체재질 : POLY PROPYLENE - 기타 부품 포함

규    격    서

ITEM NO.	품명	수량
다-11	Blue Screen	1ea

규격	세부사양	비고
세부규격	- 전동타입 - 재질 : 캔버스 배경지 - 사이즈 : (4000*6000) - 카운트 웨이트 - 모터 컨트롤러 - 캔버스롤 파이프

규    격    서

ITEM NO.	품명	수량
다-12	Auto Pole	1ea

규격	세부사양	비고
세부규격	Type : Autopole Body : Metalic Steel Length : 1.5-2.7 Meters Max weight : 1.80kg